INSTRUMENT PANEL HEAT DISTORT. REPLACE WITH NEW P/N. Chevrolet Celebrity 1987

For 1990-2009 cars

# INSTRUMENT PANEL HEAT DISTORT. REPLACE WITH NEW P/N

INSTRUMENT PANEL HEAT DISTORTED

#### VEHICLES AFFECTED: 1987 CELEBRITY -----------------

SEE ILLUSTRATION FOR THIS BULLETIN

Warpage of the instrument cluster trim pad and/or the right hand trim pad may be commented by owners and/or dealers.

This condition can be repaired by replacing the warped parts with new parts available through the Parts Department.

#### Parts required:

Grp. P/N Quantity Description ---- --- -------- -----------

11509709 9 Bolt/screw I/P attaching

10.235 10100339 1 I/P Tr. LH

9.743 10100330 1 Pad, I/P Cstr, Tr. (Paint to match)

10.235 10100338 1 Pad, I/P Tr. RH (W/C60) Paint to match

10.235 10100352 1 Pad I/P Tr. RH (Exc. C60) Paint to match

#### NOTICE: BOLT/SCREW, P/N 11509709, MUST BE USED WHEN REPLACING ALL TRIM PADS. BOLT/SCREW, P/N 11503396, HAS AN OIL BASED FINISH WHICH WILL CAUSE NEW TRIM PADS TO DECOMPOSE AROUND ATTACHMENTS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.