FELT MATERIAL ON I/P TRIM PLATE LOOSE. Chevrolet Celebrity 1989

For 1990-2009 cars

# FELT MATERIAL ON I/P TRIM PLATE LOOSE

#### Model and Year: 1989 A CAR

Owners of some 1989 A Cars may comment on the felt anti-glare material becoming loose around the edges of the Instrument Panel trim plate.

#### Correction:

1. Remove trim plate.

2. Reattach felt material using 3M Trim Adhesive #08031 or equivalent, following manufacturer's instruction.

3. Reinstall trim panel.

Production was changed with the start of the 1990 models.

Labor Operation Number: T1598

Labor Time: .6 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.