COMPARTMENT DOOR LOCK STRIKER NEW P/N AND INSTALL PROCEDURES. Chevrolet Celebrity 1983

For 1990-2009 cars

# COMPARTMENT DOOR LOCK STRIKER NEW P/N AND INSTALL PROCEDURES

#### Model and Year 1982-83 CELEBRITYS

When replacing the instrument panel compartment door lock striker on 1982-83 Celebritys, use P/N 14086179, striker. Install as follows:

1. Remove trim plate from I/P.

2. Remove existing striker plate.

3. Align new striker rod into corner of rabbet and against left boss.

4. Drill 3/16" diameter, two (2) holes using striker as template.

5. Attach striker with 3/16" diameter 3/8" long blind rivet as shown (see illustration), two (2) required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.