HEI MODULE CODE 42 INCORRECT HEI MODULE. Chevrolet Chevette 1981

For 1990-2009 cars

# HEI MODULE CODE 42 INCORRECT HEI MODULE

#### Subject: H.E.I. MODULES - 1981 AND 1982 MODELS

When replacing an H.E.I. module, be sure that the correct part number is being installed. 1981 and 1982 are not interchangeable. The correct module part numbers are:

1981 - 1978617

1982 - 1976908

Some of the parts ordering systems dealers utilize will mix the part numbers and ship the incorrect H.E.I. module. This is being addressed and corrected. If a 1981 H.E.I. module is installed in a 1982 system, the check engine light will come on and Code 42 will be stored.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.