PULSAIR VALVE REPLACEMENT-NEW P/N REPLACEMENT INFORMATION. Chevrolet Citation 1980

For 1990-2009 cars

# PULSAIR VALVE REPLACEMENT-NEW P/N REPLACEMENT INFORMATION

#### Model and Year 1980 CITATION WITH 2.8L ENGINE (CODE 7)

#### TO: ALL CHEVROLET DEALERS

This cancels and replaces Chevrolet Dealer Service Bulletin 80-95 dated November, 1984, which should be destroyed. The reissue includes labor operation number and labor time for the replacement operation.

If it becomes necessary to replace pulsair valves on Citations with 2.8L V6 engines, stainless steel valves should be used.

The part numbers for these new stainless steel valves are 22048268 (R.H.) and 22048269 (L.H.).

Labor Operation Number: J6180

Labor Time: Right: .6 Left: .5

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.