EXHAUST HANGER 'O-RING' UNHOOKING FROM RETAINERS. Chevrolet Corsica 1991

For 1990-2009 cars

# EXHAUST HANGER 'O-RING' UNHOOKING FROM RETAINERS

#### SUBJECT: EXHAUST HANGER 'O-RING' UNHOOKING (NEW EXHAUST HANGER O-RING)

#### VEHICLES AFFECTED: 1990-1991 'L' CORSICA/BERETTA VEHICLES

A condition may exist on some 1990-91 Corsica/Beretta vehicles where the exhaust hanger "0-rings" may become repeatedly unhooked from their retainers. This may cause more than normal looseness in the system and may cause underbody noise comments from the owner.

A new design exhaust hanger "0-ring" has been released to correct this condition. The new part number is 10056770.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.