HOOD WINDSHEILD/ WIPER ARM DAMAGE. Chevrolet Corsica 1987

For 1990-2009 cars

# HOOD WINDSHEILD/ WIPER ARM DAMAGE

#### Model and Year: 1987-88 BERETTA, CORSICA

Opening the hood past the prop rod location on the 1987-88 Corsica or Beretta may cause damage to the hood, windshield or wiper arm.

Unlike other model vehicles, this hood is not designed to open to a 80 - 90 degree position.

DO NOT Open the hood to 80 - 90 degree position when under hood service is required.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.