No Drive in All Ranges. Chevrolet Corsica 1996

For 1990-2009 cars

Checks | Cause
--- | ---
Oil Level | Incorrect level
Torque Converter (1) | The converter to flex plate bolts are missing

Oil Pressure

• | The pressure regulator valve is sticking in the bushing

• | Pump seals are worn (347, 350)

• | The oil pump shaft is broken (18)

Differential (678-687) | The differential is damaged or broken up

Drive Link (101)

• | The drive link is broken (101)

• | An object is between the drive link and the sprocket (101, 103, 122)

Manual Valve (406) | A retainer clip is fallen out (441)
Manual Linkage (701-704) | Misadjusted
Input Shaft (624) | The shaft is loose or has broken away from the forward clutch drum
Reaction Carrier (665) | The carrier is broken at the lo roller clutch cam (662, 665)
Forward Clutch Housing | Forward Housing