SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL. Chevrolet Corsica 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3C FRONT SUSPENSION (INNER HUB SEAL INSTALLER ART WORK LABELED WITH CORRECT TOOL NUMBER)

#### VEHICLES AFFECTED:1991 J/N/L/ CARS

The 1991 J, L and N Service Manual improperly labels the Inner Hub Seal Installer. The correct tool number is J34658.

The following art for this tool #J34658 replaces the current art shown. Reference to the tool number must also be corrected on the following pages in the text.

PAGES Division Carline TEXT ILLUSTRATION ----------- ------------ --------- ----------- 3C-7, 3C-8 3C-14 Chevrolet J 3C-9, 3C-10 3C-15 Chevrolet L

3C-7, 3C-8 3C-14 Pontiac J 3C-8, 3C-10 3C-16 Pontiac N

3C-8, 3C-10 3C-16 Oldsmobile N

3C-8, 3C-10 3C-16 Buick N

Please correct your copies of the Service Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.