CAMPAIGN: FRONT SHOULDER BELT RETRACTOR (SUPPLEMENT). Chevrolet Corsica 1990

For 1990-2009 cars

# CAMPAIGN: FRONT SHOULDER BELT RETRACTOR (SUPPLEMENT)

#### Subject: PRODUCT SAFETY CAMPAIGN 90C36(a)-FRONT SHOULDER BELT RETRACTOR

-- SUPPLEMENT --

#### Model and Year: 1988-90 CHEVROLET CORSICA AND BERETTA W/PASSIVE RESTRAINT SYSTEM

#### To: All Chevrolet Dealers

THIS BULLETIN REVISES THE SERVICE PROCEDURE AND CLAIM INFORMATION SECTIONS OF CHEVROLET PRODUCT SAFETY CAMPAIGN BULLETIN 90C36 ISSUED DECEMBER, 1991. SPECIFICALLY, AN INSPECTION TO DETERMINE IF THE VEHICLE HAS A PASSIVE (DOOR MOUNTED) OR ACTIVE ("B" PILLAR MOUNTED) SAFETY BELT SYSTEM HAS BEEN ADDED (LABOR OPERATION V7193 WILL COVER THE INSPECTION). ALSO, LABOR OPERATION V7192 HAS BEEN ADDED TO PROVIDE A SEPARATE CLAIM OPTION FOR CORSICA MODEL VEHICLES WITHOUT COMFORT FEATURE ("WINDOW SHADE") SAFETY BELTS. LABOR OPERATION V7191 WILL BE USED FOR CORSICA MODEL VEHICLES WITH COMFORT FEATURE ("WINDOW SHADE") SAFETY BELTS. INVOLVED VEHICLE LISTINGS FOR THIS CAMPAIGN ARE ENCLOSED WITH THIS SUPPLEMENT.

#### SERVICE PROCEDURE (ADDITION)

For Corsica and Beretta:

#### INSPECTION PROCEDURE

Inspect vehicle for the presence of an active or passive safety belt system. on vehicles equipped with active belt systems, the front lap and shoulder belt retractors are located in the "B" pillar (or front door striker pillar) and the shoulder belt upper guide loop is attached to the top of the "B" pillar. on vehicles equipped with passive belt systems, the front lap and shoulder belt retractors are located in the front doors and the shoulder belt upper guide loop is attached to the door in the upper rear corner of the front door glass opening.

If the vehicle is found to have a passive safety belt system (door mounted), proceed with the service procedure portion of the bulletin.

If the vehicle is found to have an active safety belt system ("B" pillar mounted), do not attempt to perform the service procedure. The vehicle owner should be informed that his/her vehicle was inadvertently included in the campaign and that no service will be required. Apply a Campaign Identification Label and return the vehicle to the owner. File labor operation V7193 for vehicles which require inspection only.

#### CLAIM INFORMATION (REVISED)

Submit a Product Campaign Claim with the information indicated below:

* FAILED PARTS CC-FC LABOR LAB OTH REPAIR PERFORMED PC PART NO. ALLOW OP HRS HRS --------------------------------------------------------------------------- Replace Both Front Seat Shoulder Belt Retractors - Coupe 1 12515769 ** SK-00 V7190 1.1 0.1 - With Comfort Feature

Replace Both Front Seat Shoulder Belt Retractors - Sedan 1 12515771 ** SK-00 V7191 1.4 0.1 - With Comfort Feature

Replace Both Front Seat Shoulder Belt Retractors - Sedan 1 12515770 ** SK-00 V7192 1.4 0.1 - Without Comfort Feature

Inspect - Vehicle Has An Active Belt -- --- -- SK-00 V7193 0.2 0.1 System - No Further Action Required

* Campaign Administrative Allowance.

** The "Parts Allowance" should be the sum total of the current GMSPO Dealer Net price plus 30% of all parts required for the repair.

Dealers will automatically receive the correct labor and material allowance based on the labor operation performed.

Refer to the Chevrolet Claims Processing Manual for details on Product Campaign Claim Submission.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.