RATTLE OR ITCH BETWEEN DEFROSTER GRILLE. Chevrolet Corsica 1995

For 1990-2009 cars

# RATTLE OR ITCH BETWEEN DEFROSTER GRILLE

#### SUBJECT: RATTLE OR ITCH BETWEEN DEFROSTER GRILLE AND INSTRUMENT PANEL (PLACE BUTYL BETWEEN DEFROSTER GRILLE AND I/P)

#### MODELS: 1993-96 CHEVROLET BERETTA, CORSICA

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE DEFROSTER GRILLE MAY RATTLE OR ITCH AGAINST THE INSTRUMENT PANEL.

#### CAUSE:

CLOSE TOLERANCES WITHOUT ENOUGH RETAINING FORCE MAY BE ALLOWING MOVEMENT OF THE DEFROSTER GRILLE CAUSING AN ITCH OR RATTLE.

#### CORRECTION:

PLACE TWO PIECES OF BUTYL BETWEEN THE INSTRUMENT PANEL AND DEFROSTER GRILLE, ONE ON EACH SIDE OF THE AIR VENT AS INDICATED IN FIGURE 1.

LEFT SIDE: PLACE BUTYL 15MM (19/32") RIGHT OF THE VIN PLATE AND 10MM (13/32") REARWARD OF THE WINDSHIELD.

RIGHT SIDE: PLACE BUTYL 70MM (2 3/4") RIGHT OF THE INBOARD RETAINING CLIP AND 10MM (13/32") REARWARD OF THE WINDSHIELD.

FIGURE 1: 1. INSTRUMENT PANEL 2. DEFROSTER GRILLE 3. VIN PLATE 4. RH INBOARD RETAINING CLIP 5. APPROXIMATE LOCATION OF BUTYL

#### PROCEDURE:

1. REMOVE DEFROSTER GRILLE WITH A BLUNT TOOL TO ELIMINATE DAMAGE TO THE INSTRUMENT PANEL (BEGIN REMOVAL FROM THE RIGHT SIDE OF THE INSTRUMENT PANEL).

2. INSTALL BUTYL (REFER TO FIGURE 1 AND ABOVE TEXT FOR PROPER POSITIONING).

3. INSTALL DEFROSTER GRILLE (BEGIN INSTALLATION FROM THE LEFT SIDE OF THE INSTRUMENT PANEL).

#### IMPORTANT: WHEN REMOVING A DEFROSTER GRILLE WITH BUTYL IN PLACE, TAKE CARE NOT TO GET THE BUTYL ON THE INSTRUMENT PANEL TOPPER PAD.

#### PARTS INFORMATION:

P/N 22653673 - INSULATOR, INSTRUMENT PANEL TRIM PAD (BUTYL)

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: D1406 LABOR TIME: 0.2 HR (GRILLE, DEFROSTER OUTLET - REPLACE, CENTER) ADD: 0.1 HR (TO REMOVE/CLEAN BUTYL FROM I/P AND DEFROSTER GRILLE) ADD: 0.1 HR (TO INSTALL TWO PIECES OF BUTYL) ADD: 0.4 HR (TO COLOR COAT, MATERIAL ALLOWANCE - GB)

FIGURES: 01 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.