Fastener Tightening Specifications. Chevrolet Corsica 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Accelerator Cable Mounting Bracket | 25 | 18 | --
Accessory Bracket Assy. to Block Bolts | 50 | 37 | --
Camshaft Sprocket | 130 | 96 | --
Camshaft Position Sensor to Block Bolt | 10 | -- | 89
Camshaft Thrust Plate | 12 | -- | 106
Connecting Rod Cap Nuts | 52 | 38 | --
Coolant Drain Plug - Cylinder Block | 15 | 11 | --
Coolant Outlet | 10 | -- | 89
Coolant Pump | 25 | 18 | --
Coolant Pump Inlet | 25 | 18 | --
Crankcase Front Cover Bolts | 11 | -- | 97
Crankshaft Main Bearing Cap Bolts | 95 | 70 | --
Crankshaft Pulley to Hub Bolt | 50 | 37 | --
Crankshaft Pulley Hub to Crankshaft Bolts | 105 | 77 | --
Crankshaft Sensor | 11 | -- | 97
Cylinder Head Bolts -- Long | 63 + 90 degrees | 46 + 90 degrees | --
Cylinder Head Bolts -- Short | 58 + 90 degrees | 43 + 90 degrees | --
Direct Ignition System Coil Assembly | 25 | 18 | --
EGR Valve Adapter | 11 | -- | 97
EGR Valve | 26 | 19 | --
Engine Lift Bracket Bolt | 50 | 37 | --
Engine Lift Bracket Nut | 50 | 37 | --
Engine Mount Strut Bolts | 100 | 74 + 90 degrees | --
Engine Mount Strut Bracket Bolts (Rear) | 75 | 55 | --
Engine Mount Strut Bracket Bolts (Front) | 66 | 49 | --
Engine Mount Assembly Cage Nuts | 45 | 33 | --
Engine Mount Assembly-to-Body Nuts | 66 | 49 | --
Engine Mount Assembly-to-Drive Belt Tensioner Bracket Bolts | 60 | 44 + 90 degrees | --
Exhaust Manifold Nuts | 30 | 22 | --
Flywheel Bolts | 75 | 55 | --
Lower Intake Manifold Nuts | 33 | 24 | --
Lower Intake Manifold Studs | 10 | -- | 89
Upper Intake Manifold Bolts | 30 | 22 | --
Lifter Guide | 11 | -- | 97
MAP Sensor | 3 | -- | 27
Oil Fill Tube | 12 | -- | 106
Oil Filter | 17 | 13 | --
Oil Filter Adapter | 35 | 26 | --
Oil Pan | 10 | -- | 89
Oil Pump Cover Bolts | 10 | -- | 89
Oil Pump Drive Assembly | 25 | 18 | --
Oil Pump Mounting Bolt | 44 | 32 | --
Oxygen Sensor | 42 | 31 | --
PCV Valve Cap | 10 | -- | 89
Power Brake Hose Vacuum Fitting | 13 | -- | 115
Rocker Arm Nuts | 30 | 22 | --
Rocker Arm Studs | 50 | 37 | --
Rocker Arm Cover Bolts | 10 | -- | 89
Serpentine Drive Belt Bracket Bolt | 50 | 37 | --
Serpentine Drive Belt Tensioner Bolt | 50 | 37 | --
Spark Plugs | 17 | 13 | --
Timing Chain Tensioner Bolts | 24 | 18 | --