Engine Controls Components. Chevrolet Corsica 1996

For 1990-2009 cars

Name | Location | Locator View (8A Cell 201 Page #) | Figure | Connector Eng View
--- | --- | --- | --- | ---
24X Crankshaft Position (CKP) Sensor | Lower right side of engine | 4 | 8 | --
7X Crankshaft Position (CKP) Sensor | Lower right side of engine | 4 | 8 | --
A/C Compressor Relay | Right side engine compartment | 5 | 10 | 202-38
A/C Refrigerant Pressure Sensor | Right hand side of engine compartment | 8 | 15 | --
Camshaft Position (CMP) Sensor | Right hand side of engine, below cover | 5 | 9 | --
Data Link Connector (DLC) | On bottom of Instrument Panel, right of steering column | 19 | 37 | 202-11
Engine Coolant Temperature (ECT) Sensor | Top left hand side of engine | 5 | 9 | --
Evaporative Canister Purge Solenoid Valve | Rear of Engine | 2 | 4 | --
Evaporative Purge Vacuum Switch | LH rear of engine | 2 | 4 | --
Exhaust Gas Recirculation (EGR) Valve | Upper left hand side of engine | 3 | 6 | 202-40
Fuel Injectors | Top of engine, mounted to fuel rail, at each cylinder intake port | 5 | 9 | --
Fuel Pressure Regulator | Mounted on the Fuel Injector Rail, top, left hand side of engine | -- | -- | --
Fuel Pump/Fuel Level Sender | Mounted inside fuel tank | 14 | 27 | --
Fuel Pump Relay | Right hand side engine compartment | 5 | 10 | 202-41
Fuse Block | LH side of Instrument Panel | 18 | 35 | --
Generator | Top center right hand side of engine | 3 | 6 | 202-42
Heated Oxygen sensor 1 (HO2S1) | Rear of engine, in exhaust manifold | 3 | 6 | 202-41
Heated Oxygen sensor 2 (HO2S2) | In exhaust system, behind Catalytic Converter | 6 | 11 | 202-44
Idle Air Control Valve (IAC) | Top of engine, front of Throttle Body Assembly | 4 | 7 | 202-42
Ignition Control Module (ICM) | Top right hand front of engine | 3 | 6 | 202-40
Intake Air Temperature (IAT) Sensor | Left hand front of engine compartment, on air intake duct | 4 | 7 | --
Knock Sensor (KS) | Front of engine, above starter | 4 | 8 | --
Malfunction Indicator Lamp (MIL) | Upper right hand side of Instrument Panel | -- | Refer to I/P diagnosis | --
Manifold Absolute Pressure (MAP) Sensor | Top rear of engine, on intake manifold | 1 | 2 | --
Mass Air Flow (MAF) Sensor | Left hand front of engine compartment, in air cleaner duct | 11 | 21 | --
Powertrain Control Module (PCM) | Right hand side of lower I/P | 6 | 12 | 202-29
Positive Crankcase Ventilation Valve | Top, right hand, center of engine, below Manifold Absolute Pressure (MAP) Sensor | -- | -- | --
Primary Cooling Fan | Front center of engine compartment | 8 | 16 | --
Primary Cooling Fan Relay | Right hand side of engine compartment | 5 | 10 | 202-41
SMCC II Cruise Control Module | Left hand rear of engine compartment, center front of dash | 5 | 10 | 202-10
Throttle Body | Mounted to the Upper Intake Manifold, top, left hand side of engine | -- | -- | --
Throttle Position (TP) Sensor | Top of engine, on Throttle Body Assembly | 4 | 7 | --
TCC Brake Switch | Lower left hand side of I/P | 18 | 36 | --
Transaxle Range Switch / Park Neutral Position (PNP) Switch | Rear left hand side of engine compartment, mounted to top of transaxle | 2 | 4 | 202-23
Vehicle Speed Sensor (VSS) | Lower right hand of engine on Transaxle | 2 | 4 | --