BRAKE DRAG-(MAY BE MISADJUSTED BRAKE LIGHT SWITCH). Chevrolet Corsica 1988

For 1990-2009 cars

# BRAKE DRAG-(MAY BE MISADJUSTED BRAKE LIGHT SWITCH)

#### VEHICLES AFFECTED: 1987-88 L-CAR

This bulletin replaces Bulletin #88-5-103, 88-8-111.

Condition: The brakes may stay slightly applied on the 1987-88 L-car, causing brake drag. Depending on the amount of the apply force, the results may range from early brake pad and rotor wearout, to decreased brake pad life.

Cause: The brake lamp switch may be holding the brake pedalslightly applied. The switch retaining clip may not allow the switch to return to its correct position by the usual adjustment procedure of pulling up on the brake pedal.

#### Correction:

1. Pull up (rearward) on the brake pedal, with a force of 65-90 N.m. (15-20 lbs.). If no "click" is heard, perform steps 2 through 4.

2. Remove the hush panel.

3. Move brake switch rearward, far enough in the clip so that the brake pedal returns to its normal position. If the switch is difficult to move rearward, remove the switch completely. Then remove and discard the retaining clip. Reinstall a new clip, P/N 22534155, insuring that neither of the tabs go into the slot i n the switch mounting bracket hole (See Figure 1).

Parts are currently available from GMPARTS

4. Reinstall the switch into the retaining Clip, and adjust the switch by pulling rearward on the brake pedal until there is a small gap (less than 1/16") between the end of the threaded switch barrel and the brake pedal bracket (See Figure 2). A normally adjusted switch will have no gap; however, a small gap will insure that the brake pedal is not being held in. Check the brake lamps and cruise control system for proper operation.

Use Existing Labor Operations.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.