OIL FILTER REPLACEMENT UPDATE INFORMATION ON CORRECT FILTERS. Chevrolet Corsica 1991

For 1990-2009 cars

# OIL FILTER REPLACEMENT UPDATE INFORMATION ON CORRECT FILTERS

#### Subject: CORRECT OIL FILTER

#### Model and Year: 1987-89 CORSICA, BERETTA WITH 2.8L ENGINE 1990-91 CORSICA, BERETTA WITH 3.L L ENGINE

This bulletin advises dealers and customers of the correct replacement oil filter for the specified vehicles. Disregard information contained in the 1987-91 Corsica/Beretta Owners Manuals and Parts Catalogs showing the AC-TYPE PF-51 as the replacement oil filter. The proper replacement oil filter for the specified vehicles is an AC TYPE PF-40. The AC TYPE PF-51 extends below the suspension and may be damaged by stones, rocks, or road hazards. The AC TYPE PF-40 is shorter and does not extend below the suspension.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.