PUNCTURED AIR CONDITIONING CONDENSER - NO COOLING. Chevrolet Corsica 1988

For 1990-2009 cars

# PUNCTURED AIR CONDITIONING CONDENSER - NO COOLING

#### MODEL AND YEAR: 1987-88 BERETTA, CORSICA

The air conditioning condensers in some 1987-88 Beretta, Corsica models may have been punctured by a screw from the lower air deflector (See Figure 1).

For this reason, future production parts will eliminate the inboard attachments. Likewise, do not install the two inboard screws when installing the air deflector at the dealership. The current installation instructions supplied earlier are incorrect. New installation instructions are immediately forthcoming.

If an interference is noted between the condenser and deflector attaching screw on the subject vehicles, remove the two inboard screws.

Labor Operation Labor Number Time ------ ----- Remove two inboard attaching screws: D9990 .2 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.