BINDING OR POPPING FRT. DOOR GLASS (REPAIR PROCEDURE). Chevrolet Corsica 1992

For 1990-2009 cars

# BINDING OR POPPING FRT. DOOR GLASS (REPAIR PROCEDURE)

REVISION: 09/06/94

THIS BULLETIN IS BEING REVISED TO ADD 1990-95 MODEL YEARS. PREVIOUS DIVISIONAL PUBLICATION NUMBERS WERE:

CHEVROLET 89-131-10 GM OF CANADA 89-2-149 ********************************************************************

#### SUBJECT: BINDING OR POPPING FRONT DOOR GLASS/ROAD NOISE (ADJUST STABILIZER)

#### MODELS: 1988-95 CHEVROLET BERETTA AND CORSICA

#### CONDITION:

SOME OWNERS MAY COMMENT ON A BINDING OR POPPING NOISE ON THE FRONT DOOR GLASS WHEN THE GLASS IS INITIALLY ROLLED DOWN, OR ROAD NOISE CAUSED BY A GAP BETWEEN THE FRONT DOOR GLASS AND INNER BELT SEALING STRIP WITH THE GLASS IN FULL UP POSITION.

#### CAUSE:

THE CONDITIONS MAY BE CAUSED BY A MISADJUSTED REGULATOR ARM STABILIZER PLATE.

CORRECTION: (SEE ILLUSTRATION)

THE STABILIZER MAY BE ADJUSTED INBOARD OR OUTBOARD BY BENDING WITH LOCKING PLIERS. IT MAY BE CONSIDERED TO BE ADJUSTED PROPERLY WHEN:

1. THERE IS ENOUGH INBOARD PRESSURE TO PREVENT GLASS MOVING OUTBOARD, CREATING GAPS OF INNER BELT STRIP TO GLASS, BUT;

2. NOT SO MUCH INBOARD PRESSURE TO INCREASE BINDING OF THE REGULATOR ARM TO THE STABILIZER.

3. AFTER NECESSARY ADJUSTMENT HAS BEEN COMPLETED, LIGHTLY COAT THE OUTBOARD SURFACE OF THE REGULATOR ARM AND THE INBOARD SURFACE OF THE STABILIZER ARM WHERE THEY COME IN CONTACT WITH LUBRIPLATE GM P/N 1052196 OR EQUIVALENT.

#### PARTS AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

LABOR OPERATION NUMBER: C0100 (RH) C0101 (LH) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.