SERVICE MANUAL UPDATE-SEC. 6E3 WIRE COLOR REVISIONS. Chevrolet Corsica 1992

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 6E3 WIRE COLOR REVISIONS

#### subject: WIRE COLOR REVISIONS

#### Model and Year: 1992-93 CORSICA AND BERETTA WITH 3.1 L ENGINE

This Bulletin revises wire colors for Circuits 455 and 410 on pages 6E3-A3, 6E3-A34 and 6E3-A36 of the 1992 3.1L (VIN T) "L" carline. The revised wire colors are:

- CTS Pin A, Circuit 455 ..... PPL - CTS Pin B, Circuit 410 ..... YEL

Revised wire color for Circuit 410 on pages 6E3-A38 and 6E3-A40 of the 1993 3.1 L (VIN T) "L" carline is:

- ECT Pin B, Circuit 410 ..... YEL

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.