Shift Speed. Chevrolet Corsica 1996

For 1990-2009 cars

#### 3T40 Shift Speed Chart '96 L Car

Transmission Model | 6AKC
--- | ---
Vehicle Series | L
Engine Displacement | 2.2L
Engine RPO Code | LN2
Engine VIN Code | 4
Overall Axle Ratio | 3.18
Final Drive Ratio | 2.84
Drive/Driven Sprocket Teeth | 33/37
Minimum Throttle 1-2 Upshift | 11
Wide Open Throttle 1-2 Upshift | 41
Minimum Throttle 2-3 Upshift | 21
Wide Open Throttle 2-3 Upshift | 76
Minimum TCC Apply | 35
N/V Ratio | 45
Torque Converter K-Factor | 203
Governor Pressure Switch | N/A
Second Gear Pressure Switch | N/A
Third Gear Pressure Switch | N.O.
Direct Clutch Type | 5 plate
Transmission Vent Type | Elbow
Manual Valve Thermal Element | NO

• | N/A = Not Available

• | N.O. = Normally Open

• | N/V Ratio = Engine RPM to Vehicle Speed ratio in the third gear with TCC applied

• | K-Factor = Torque converter numeric rating (combines stall speed and torque multiplication ratings)

• | Speeds are indicated in Miles Per Hour (mph). Mph = km/h x 1.609