Vehicle Speed Sensor Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Remove the vehicle speed sensor (VSS) lead from the transmission.
3. Remove the vehicle speed sensor housing bolts.
4. Remove the vehicle speed sensor housing.
5. Remove the speed sensor housing.

### Installation Procedure

1. Install the speed sensor housing O-ring.
2. Lubricate the O-ring with DEXRON®-IIE or DEXRON®-III.
3. Install the speed sensor housing.
4. Install the speed sensor bolts.
5. Install the VSS lead to the transmission.
6. Lower the vehicle.