Fastener Tightening Specifications. Chevrolet Corsica 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Resonator Upper Attaching Bolt | 6 | -- | 54
A/C Refrigerant Sensor | 4.75 | -- | 42
Accelerator Cable Bracket Nut | 30 | 22 | --
Accelerator Cable Bracket Bolts | 25 | 18 | --
Air Cleaner Cover Screws | 3 | -- | 31
Air Cleaner Outlet Duct Clamps | 5 | -- | 45
Air Cleaner Outlet Resonator Clamp | 5 | -- | 45
CKP Sensor Bolts | 8 | -- | 71
CMP Sensor Bolts | 8 | -- | 71
ECT Sensor | 25 | -- | 18
EGR Valve Bolts | 26 | 19 | --
EVAP Canister Retainer Attaching Bolt | 10 | 7 | --
Fuel Filter Fitting | 27 | 20 | --
Fuel Line Fitting to Fuel Rail | 27 | 20 | --
Fuel Line Fitting to Fuel Rail Nut (2.2L) | 30 | 22 | --
Fuel Inlet Retaining Nut | 30 | 22 | --
Fuel Inlet Retaining Nut | 10 | -- | 89
Fuel Line Clamp Screws | 10 | -- | 89
Fuel Pressure Regulator Screw | 3.5 | -- | 31
Fuel pump and Engine Oil Pressure Switch | 12 | 9 | 112
Fuel Return Pipe Nut | 30 | 22 | --
Headlamp Assembly Retaining Screws | 6 | -- | 53
HO2S 2 | 41 | 30 | --
ICM Cover Bolts | 22 | 16 | --
Idle Air Control Valve Screws | 3.0 | -- | 27
Ignition Coil Retaining Screws | 4.5 | -- | 40
Ignition Coil Assembly Attaching Bolts | 25 | 18 | --
Injector Retaining Bracket Screws | 3.5 | -- | 31
KS Module Cover Screws | 3 | -- | 27
Knock Sensor | 19 | 14 | --
Knock Sensor Module Cover | 5 | -- | 44
Lower Manifold Assembly Nuts | 30 | 22 | --
MAP Sensor Attaching Screw | 6 | -- | 53
Muffler Hanger Bolt | 15 | 11 | --
Oil Level Attaching Bolt | 10 | -- | 88
O2S 1 | 41 | 30 | --
PCM Retainer Attaching Bolts | 10 | -- | 88
Purge Valve Mounting Bracket Attaching Bolt | 8 | -- | 70
Regulator Retainer Screw | 6 | -- | 53
Resonator Upper Attaching Bolt | 6 | -- | 53
Tank Retaining Straps Bolt | 35 | 26 | --
Throttle Position (TP) Sensor Screws | 2.0 | -- | 18
TP Sensor Mounting Screws | 3 | -- | 27
Upper Manifold Assembly Studs/Bolts | 30 | 22 | --