Transmission Control Lever Knob Replacement. Chevrolet Cruze (SGM) 2009

For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the transmission control lever boot from the transmission control lever. Refer to CELL LINK.

1

Transmission Control Lever Knob

#### Procedure

Release the clip from the transmission control lever by pressing from the side. The groove is on the left side of the transmission control lever and is not visible.