CAMPAIGN: NON-CALIF. ENGINES REVISED MAINTENANCE SCHEDULE. Chevrolet El Camino 1980

For 1990-2009 cars

# CAMPAIGN: NON-CALIF. ENGINES REVISED MAINTENANCE SCHEDULE

THE MAINTENANCE SCHEDULE INCLUDED WITH THE 1980 TURBOCHARGED EQUIPPED CHEVROLET MONTE CARLOS SPECIFIED A 30,000 MILE INTERVAL BETWEEN SPARK PLUG CHANGES INSTEAD OF THE CURRENT 22,500 MILE INTERVAL.

TO CORRECT THIS ERROR, WE ARE SENDING A NEW CORRECT MAINTENANCE SCHEDULE, P/N 14021722A DIRECTLY TO AFFECTED OWNERS OF RECORD. REFER TO COPY OF OWNER'S LETTER INCLUDED WITH THIS BULLETIN.

IF YOUR DEALERSHIP WAS SHIPPED VEHICLES INVOLVED IN THIS PROGRAM, YOU WILL RECEIVE A VEHICLE IDENTIFICATION NUMBER LIST OF THESE VEHICLES AND A MAINTENANCE SCHEDULE FOR EACH VEHICLE FOR WHICH NO OWNER OF RECORD IS LISTED.

THIS NEW FOLDER IS TO BE PLACED IN THE GLOVE BOX OF VEHICLES IN STOCK AND THE ORIGINAL FOLDER DISCARDED. IF A VEHICLE HAS BEEN DELIVERED AND THE OWNER'S NAME IS NOT ON THE VEHICLE IDENTIFICATION NUMBER LIST, FORWARD A NEW FOLDER TO THE OWNER.

VEHICLES INVOLVED

1980 CHEVROLET MONTE CARLOS EQUIPPED WITH V-6 NON-CALIFORNIA ENGINES WITHIN THE FOLLOWING VEHICLE IDENTIFICAITON NUMBER PARAMETERS: PLANT FROM THROUGH

DORAVILLE 1Z373AD400001 1Z373AD427673 ARLINGTON 1Z373AR400001 1Z373AR423803 LEEDS 1W35KAK400001 1W35KAK464496 FREMONT 1Z373AZ400001 1Z373AZ408039

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.