Restraint, Panel, Cushion, Frame - Driver Seat. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Drivers Front Seat. Refer to Seat Replacement - Front Bucket (Link disabled for test). Drivers Front Seat Belt Buckle. Refer to Seat Belt Buckle Replacement - Front (Link disabled for test). Lumber Support Knob. Refer to Lumber Support Knob Replacement (Link disabled for test).
1 | Restraint, Driver Seat Head
2 | Guide, Driver Seat Head Restraint Tip: Press the tabs on the bottom of the guide in while pushing up.
3 | Retainers, Driver Seat Back Panel
4 | Panel, Driver Seat Back Tip: Disengage the retainers by pulling the panel from the seat back frame.
5 | Frame, Driver Seat Back
6 | Cushion and Pad, Driver Seat Tip: Remove the rear retainers and J-strips from the seat frame and recliner rod.
7 | Cushion and Pad, Driver Seat Back Tip: Remove the J-strips from the seat frame.