Inline Harness Connector End Views. Chevrolet Evaluator 1985

For 1990-2009 cars

## Inline Harness Connector End Views Non-test

Table 1: | C100 Engine Harness to Automatic Transmission Harness
Table 2: | C101 LF Wheel Speed Sensor Jumper Harness to Body Harness (JL9)
Table 3: | C102 RF Wheel Speed Sensor Jumper Harness to Body Harness (JL9)
Table 4: | C108 Engine Harness to Body Harness (LX9)
Table 5: | C109 Forward Lamp Harness to Left Headlamp Harness
Table 6: | C110 Forward Lamp Harness to Right Headlamp Harness
Table 7: | C130 Engine Harness to Fuel Injector Harness (L61)
Table 8: | C130 Engine Harness to Fuel Injector Harness (LX9)
Table 9: | C206 I/P Harness to Body Harness
Table 10: | C207 I/P Harness to Body Harness
Table 11: | C208 I/P Harness to Body Harness
Table 12: | C214 Body Harness to Console Harness (w/o UK6, U32)
Table 13: | C214 Body Harness to Console Harness (UK6, U32)
Table 14: | C300 Body Harness to Drivers Seat Harness
Table 15: | C304 Body Harness to LF Pretensioner Jumper Harness
Table 16: | C305 Body Harness to RF Pretensioner Jumper Harness
Table 17: | C310 Body Harness to Passenger Seat Harness
Table 18: | C315 Video Screen Harness to DVD Jumper Harness
Table 19: | C319 Body Harness to Left Inflatable Restraint Side Impact Module Jumper Harness (AY1)
Table 20: | C320 Body Harness to Right Inflatable Restraint Side Impact Module Jumper Harness (AY1)
Table 21: | C403 Body Harness to Rear Wheel Speed Sensor Harness (JL9)
Table 22: | C404 Liftgate Harness to Body Harness (Extended Sedan)
Table 23: | C413 Fuel Sender Harness to Body Harness
Table 24: | C500 Body Harness to Left Front Door Harness
Table 25: | C600 Body Harness to Right Front Door Harness
Table 26: | C651 Headliner Harness to Body Harness
Table 27: | C700 Body Harness to Left Rear Door Harness
Table 28: | C707 Rear Lamp Harness to Left Tail Lamp Harness
Table 29: | C800 Body Harness to Right Rear Door Harness
Table 30: | C807 Rear Lamp Harness to Right Tail Lamp Harness

#### C100 Engine Harness to Automatic Transmission Harness

Connector Part Information

• | 12160493

• | 20-Way F Micro-Pack 100 Series (GY)

Connector Part Information

• | 12160782

• | 20-Way M Micro-Pack 100 Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 1222 | 1-2 Shift Solenoid Valve Control | A | L-GN | 1222 | 1-2 Shift Solenoid Valve Control
B | YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | B | YE | 1223 | 2-3 Shift Solenoid Valve Control
C | OG/BK | 1228 | PC Solenoid Valve High Control | C | PU | 1228 | PC Solenoid Valve High Control
D | L-BU/WH | 1229 | PC Solenoid Valve Low Control | D | L-BU | 1229 | PC Solenoid Valve Low Control
E | PK | 39 | Ignition 1 Voltage | E | RD | 839 | Ignition 1 Voltage
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | YE/BK | 1227 | TFT Sensor Signal | L | BN | 1227 | TFT Sensor Signal
M | TN | 2762 | Low Reference | M | GY | 452 | Low Reference
N | -- | -- | Not Used | N | -- | -- | Not Used
P | OG | 1226 | Transmission Fluid Pressure Switch Signal C | P | OG | 1226 | Transmission Fluid Pressure Switch Signal C
R | D-BU | 1225 | Transmission Fluid Pressure Switch Signal B | R | D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
S | OG/BK | 1230 | AT ISS High Signal | S | BK | 1230 | AT ISS High Signal
T | BN | 418 | TCC PWM Solenoid Valve Control | T | TN | 418 | TCC PWM Solenoid Valve Control
U | YE | 657 | TCC Release Switch Signal | U | WH | 1804 | TCC Release Switch Signal
V | D-BU/WH | 1231 | AT ISS Low Signal | V | D-GN | 1231 | AT ISS Low Signal
W | -- | -- | Not Used | W | -- | -- | Not Used

#### C101 LF Wheel Speed Sensor Jumper Harness to Body Harness (JL9)

Connector Part Information

• | 15326801

• | 2-Way F GT 150 Series, Sealed (BK)

Connector Part Information

• | 15326806

• | 2-Way M GT 150 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 830 | Left Front Wheel Speed Sensor Supply Voltage | A | L-BU | 830 | Left Front Wheel Speed Sensor Supply Voltage
B | YE | 873 | Left Front Wheel Speed Sensor Signal | B | YE | 873 | Left Front Wheel Speed Sensor Signal

#### C102 RF Wheel Speed Sensor Jumper Harness to Body Harness (JL9)

Connector Part Information

• | 15326801

• | 2-Way F GT 150 Series, Sealed (BK)

Connector Part Information

• | 15326806

• | 2-Way M GT 150 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 872 | Right Front Wheel Speed Sensor Supply Voltage | A | D-GN | 872 | Right Front Wheel Speed Sensor Supply Voltage
B | YE | 833 | Right Front Wheel Speed Sensor Signal | B | TN | 833 | Right Front Wheel Speed Sensor Signal

#### C108 Engine Harness to Body Harness (LX9)

Connector Part Information

• | 15326835

• | 8-Way F GT 150 Series, Sealed 4.0 (BK)

Connector Part Information

• | 15326840

• | 8-Way M GT 150 Series, Sealed 4.0 (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WH | 17 | Stop Lamp Switch Signal | A | WH | 17 | Stop Lamp Switch Signal
B | BN | 818 | Vehicle Speed Signal | B | BN | 818 | Vehicle Speed Signal
C | BN | 1271 | Low Reference | C | BN | 1271 | Low Reference
D | WH/BK | 1164 | 5-Volt Reference | D | WH/BK | 1164 | 5-Volt Reference
E | D-BU | 1161 | APP Sensor 1 Signal | E | D-BU | 1161 | APP Sensor 1 Signal
F | PU | 1272 | Low Reference | F | PU | 1272 | Low Reference
G | TN | 1274 | 5-Volt Reference | G | TN | 1274 | 5-Volt Reference
H | L-BU | 1162 | APP Sensor 2 Signal | H | L-BU | 1162 | APP Sensor 2 Signal

#### C109 Forward Lamp Harness to Left Headlamp Harness

Connector Part Information

• | 12146045

• | 5-Way F Metri-Pack 150 Series (WH)

Connector Part Information

• | 12103974

• | 5-Way M Metri-Pack 150 Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 150 | Ground | A | BK | 150 | Ground
B | YE | 712 | Left Headlamp Low Beam Supply Voltage | B | YE | 712 | Left Headlamp Low Beam Supply Voltage
C | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | C | GN | 711 | Left Headlamp High Beam Supply Voltage
D | D-BU | 5364 | Left DRL/Turn Supply Voltage | D | PU | 5364 | Left DRL/Turn Supply Voltage
E | BN | 9 | Park Lamp Supply Voltage | E | BN | 9 | Park Lamp Supply Voltage

#### C110 Forward Lamp Harness to Right Headlamp Harness

Connector Part Information

• | 12146045

• | 5-Way F Metri-Pack 150 Series (WH)

Connector Part Information

• | 12103974

• | 5-Way M Metri-Pack 150 Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 250 | Ground | A | BK | 250 | Ground
B | TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | B | YE | 312 | Right Headlamp Low Beam Supply Voltage
C | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | C | GN | 311 | Right Headlamp High Beam Supply Voltage
D | D-GN | 5365 | Right DRL/Turn Supply Voltage | D | PU | 5365 | Right DRL/Turn Supply Voltage
E | BN | 9 | Park Lamp Supply Voltage | E | BN | 9 | Park Lamp Supply Voltage

#### C130 Engine Harness to Fuel Injector Harness (L61)

Connector Part Information

• | 15326835

• | 8-Way F GT 150 Series, Sealed 4.0 (BK)

Connector Part Information

• | 15326840

• | 8-Way M GT 150 Series, Sealed 4.0 (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 1744 | Fuel Injector 1 Control | A | BK | 1744 | Fuel Injector 1 Control
B | L-GN/BK | 1745 | Fuel Injector 2 Control | B | L-GN/BK | 1745 | Fuel Injector 2 Control
C | PK/BK | 1746 | Fuel Injector 3 Control | C | PK/BK | 1746 | Fuel Injector 3 Control
D | L-BU/BK | 844 | Fuel Injector 4 Control | D | L-BU/BK | 844 | Fuel Injector 4 Control
E | PK | 839 | Ignition 1 Voltage | E | PK | 839 | Ignition 1 Voltage
F | OG/BK | 469 | Low Reference | F | OG/BK | 469 | Low Reference
G | L-GN | 432 | MAP Sensor Signal | G | L-GN | 432 | MAP Sensor Signal
H | GY | 2704 | 5-Volt Reference | H | GY | 2704 | 5-Volt Reference

#### C130 Engine Harness to Fuel Injector Harness (LX9)

Connector Part Information

• | 15326084

• | 16-Way F GT 150, 280 Series, Sealed (BK)

Connector Part Information

• | 15326085

• | 16-Way M GT 150, 280 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK | 839 | Ignition 1 Voltage | A | PK | 639 | Ignition 1 Voltage
B | YE | 410 | ECT Sensor Signal | B | YE | 410 | ECT Sensor Signal
C | TN | 1744 | Fuel Injector 1 Control | C | BK | 1744 | Fuel Injector 1 Control
D | L-GN/BK | 1745 | Fuel Injector 2 Control | D | L-GN/BK | 1745 | Fuel Injector 2 Control
E | PK/BK | 1746 | Fuel Injector 3 Control | E | PK/BK | 1746 | Fuel Injector 3 Control
F | L-BU/BK | 844 | Fuel Injector 4 Control | F | L-BU/BK | 844 | Fuel Injector 4 Control
G | TN/WH | 845 | Fuel Injector 5 Control | G | BK/WH | 845 | Fuel Injector 5 Control
H | YE/BK | 846 | Fuel Injector 6 Control | H | YE/BK | 846 | Fuel Injector 6 Control
J | -- | -- | Not Used | J | -- | -- | Not Used
K | GY | 2704 | 5-Volt Reference | K | GY | 2704 | 5-Volt Reference
L | OG/BK | 469 | Low Reference | L | OG/BK | 469 | Low Reference
M | L-GN | 432 | MAP Sensor Signal | M | L-GN | 432 | MAP Sensor Signal
N | OG | 631 | 12-Volt Reference | N | RD/WH | 812 | 12-Volt Reference
P | PK/BK | 632 | Low Reference | P | BK | 407 | Low Reference
R | BN/WH | 633 | CMP Sensor Signal | R | BN/WH | 633 | CMP Sensor Signal
S | -- | -- | Not Used | S | -- | -- | Not Used

#### C206 I/P Harness to Body Harness

Connector Part Information

• | 15317325

• | 22-Way F GT 150, 280 Series (L-GY)

Connector Part Information

• | 15317322

• | 22-Way M GT 150, 280 Series (L-GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-BU | 1162 | APP Sensor 2 Signal | A1 | L-BU | 1162 | APP Sensor 2 Signal
A2 | TN | 1274 | 5-Volt Reference | A2 | TN | 1274 | 5-Volt Reference
A3 | PU | 1272 | Low Reference | A3 | PU | 1272 | Low Reference
A4 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus + | A4 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus +
A5 | WH/BK | 644 | 10-Volt Reference (UK6) | A5 | WH/BK | 644 | 10-Volt Reference (UK6)
A6 | PK/WH | 1970 | Headlamp Low Beam Relay Control | A6 | PK/WH | 1970 | Headlamp Low Beam Relay Control
PK/WH | 1970 | Headlamp Low Beam Relay Control
A7 | BN/WH | 2517 | Keypad Red LED Signal (UE1) | A7 | BN/WH | 2517 | Keypad Red LED Signal (UE1)
A8 | L-GN/BK | 2515 | Keypad Supply Voltage (UE1) | A8 | L-GN/BK | 2515 | Keypad Supply Voltage (UE1)
A9 | GY | 655 | Cellular Microphone Signal (UE1) | A9 | GY | 655 | Cellular Microphone Signal (UE1)
A10 | -- | -- | Not Used | A10 | -- | -- | Not Used
A11 | BN/WH | 419 | MIL Control | A11 | BN/WH | 419 | MIL Control
B1 | D-BU | 1161 | APP Sensor 1 Signal | B1 | D-BU | 1161 | APP Sensor 1 Signal
B2 | WH/BK | 1164 | 5-Volt Reference | B2 | WH/BK | 1164 | 5-Volt Reference
B3 | BN | 1271 | Low Reference | B3 | BN | 1271 | Low Reference
B4 | TN | 2501 | High Speed GMLAN Serial Data Bus - | B4 | TN | 2501 | High Speed GMLAN Serial Data Bus -
B5 | PK | 5165 | Antenna 14V Switched Supply Voltage | B5 | PK | 5165 | Antenna 14V Switched Supply Voltage (Sedan)
B6 | PU | 1807 | Class 2 Serial Data | B6 | PU | 1807 | Class 2 Serial Data
B7 | YE/BK | 2516 | Keypad Green LED Signal (UE1) | B7 | YE/BK | 2516 | Keypad Green LED Signal (UE1)
B8 | D-GN/WH | 2514 | Keypad Signal (UE1) | B8 | D-GN/WH | 2514 | Keypad Signal (UE1)
B9 | BARE | 1489 | Drain Wire (UE1) | B9 | BARE | 1489 | Drain Wire (UE1)
B10 | PU | 493 | Rear Seat Audio Enable Signal (UK6) | B10 | PU | 493 | Rear Seat Audio Enable Signal (UK6)
B11 | GY | 91 | Windshield Wiper Switch Signal 2 | B11 | GY | 91 | Windshield Wiper Switch Signal 2

#### C207 I/P Harness to Body Harness

Connector Part Information

• | 15317325

• | 22-Way F GT 150, 280 Series (L-GY)

Connector Part Information

• | 15317322

• | 22-Way M GT 150, 280 Series (L-GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | TN | 201 | Left Front Speaker Output (+) | A1 | TN | 201 | Left Front Speaker Output (+)
A2 | L-GN | 200 | Right Front Speaker Output (+) | A2 | L-GN | 200 | Right Front Speaker Output (+)
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | TN/WH | 372 | Audio Common (U2K, U32) | A4 | TN/WH | 372 | Audio Common (U2K)
TN/WH | 372 | Audio Common (U32)
A5-A9 | -- | -- | Not Used | A5-A9 | -- | -- | Not Used
A10 | D-BU | 46 | Right Rear Speaker Output (+) | A10 | D-BU | 46 | Right Rear Speaker Output (+)
A11 | BN | 199 | Left Rear Speaker Output (+) | A11 | BN | 199 | Left Rear Speaker Output (+)
B1 | GY | 118 | Left Front Speaker Output (-) | B1 | GY | 118 | Left Front Speaker Output (-)
B2 | D-GN | 117 | Right Front Speaker Output (-) | B2 | D-GN | 117 | Right Front Speaker Output (-)
B3 | -- | -- | Not Used | B3 | -- | -- | Not Used
B4 | BARE | 814 | Drain Wire (U2K, U32) | B4 | BARE | 814 | Drain Wire (U2K)
BARE | 814 | Drain Wire (U32)
B5 | BN/WH | 367 | Left Audio Signal (+) (U2K, U32) | B5 | BN/WH | 367 | Left Audio Signal (+) (U2K)
BN/WH | 367 | Left Audio Signal (+) (U32)
B6 | D-GN/WH | 368 | Right Audio Signal (+) (U2K, U32) | B6 | D-GN/WH | 368 | Right Audio Signal (+) (U2K)
D-GN/WH | 368 | Right Audio Signal (+) (U32)
B7-B8 | -- | -- | Not Used | B7-B8 | -- | -- | Not Used
B9 | L-GN | 1011 | Remote Radio Control Signal (UK6) | B9 | L-GN | 1011 | Remote Radio Control Signal (UK6)
B10 | L-BU | 115 | Right Rear Speaker Output (-) | B10 | L-BU | 115 | Right Rear Speaker Output (-)
B11 | YE | 116 | Left Rear Speaker Output (-) | B11 | YE | 116 | Left Rear Speaker Output (-)

#### C208 I/P Harness to Body Harness

Connector Part Information

• | 15336476

• | 4-Way M Metri-Pack 280 Series (YE)

Connector Part Information

• | 15336478

• | 4-Way F Metri-Pack 280 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control | A1 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control
A2 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | A2 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
B1 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control | B1 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control
B2 | PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | B2 | PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

#### C214 Body Harness to Console Harness (w/o UK6, U32)

Connector Part Information

• | 15326893

• | 5-Way F GT 280 Series (BK)

Connector Part Information

• | 15326897

• | 5-Way M GT 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 8 | Instrument Panel Lamp Supply Voltage (NW7, NW9) | A | GY | 8 | Instrument Panel Lamp Supply Voltage (NW7, NW9)
B | BN/WH | 1571 | Traction Control Switch Signal (NW7, NW9) | B | BN/WH | 1571 | Traction Control Switch Signal (NW7, NW9)
C | BK | 1050 | Ground (NW7, NW9) | C | BK | 1050 | Ground (NW7, NW9)
D | RD/WH | 40 | Battery Positive Voltage | D | RD/WH | 40 | Battery Positive Voltage
RD/WH | 40 | Battery Positive Voltage
E | BK | 1150 | Ground | E | BK | 1150 | Ground
BK | 1150 | Ground

#### C214 Body Harness to Console Harness (UK6, U32)

Connector Part Information

• | 15304908

• | 30-Way F GT 150, 280 Series (BK)

Connector Part Information

• | 15326762

• | 30-Way M GT 150, 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | 116 | Left Rear Speaker Output (-) | A1 | YE | 116 | Left Rear Speaker Output (-)
A2 | BN | 199 | Left Rear Speaker Output (+) | A2 | BN | 199 | Left Rear Speaker Output (+)
A3 | L-BU | 115 | Right Rear Speaker Output (-) | A3 | L-BU | 115 | Right Rear Speaker Output (-)
A4 | D-BU | 46 | Right Rear Speaker Output (+) | A4 | D-BU | 46 | Right Rear Speaker Output (+)
A5 | PU | 493 | Rear Seat Audio Enable Signal | A5 | PU | 493 | Rear Seat Audio Enable Signal (UK6)
A6 | WH/BK | 644 | 10-Volt Reference (UK6) | A6 | WH/BK | 644 | 10-Volt Reference (UK6)
A7 | RD/WH | 40 | Battery Positive Voltage | A7 | RD/WH | 40 | Battery Positive Voltage
RD/WH | 40 | Battery Positive Voltage
A8 | -- | -- | Not Used | A8 | -- | -- | Not Used
A9 | BK | 1150 | Ground | A9 | BK | 1150 | Ground
BK | 1150 | Ground
A10 | BN | 9 | Park Lamp Supply Voltage | A10 | BN | 9 | Park Lamp Supply Voltage (UK6)
A11-A12 | -- | -- | Not Used | A11-A12 | -- | -- | Not Used
A13 | D-GN | 5060 | Low Speed GMLAN Serial Data | A13 | D-GN | 5060 | Low Speed GMLAN Serial Data
A14 | BK | 1050 | Ground (UK6, U32) | A14 | BK | 1050 | Ground (UK6, U32)
A15 | RD/WH | 1240 | Battery Positive Voltage | A15 | RD/WH | 1240 | Battery Positive Voltage
B1 | L-GN | 1011 | Remote Radio Control Signal | B1 | L-GN | 1011 | Remote Radio Control Signal (UK6)
B2 | BARE | 814 | Drain Wire (U32) | B2 | BARE | 814 | Drain Wire (U32)
B3 | BN/WH | 367 | Left Audio Signal (+) (U32) | B3 | BN/WH | 367 | Left Audio Signal (+) (U32)
B4 | D-GN/WH | 368 | Right Audio Signal (+) (U32) | B4 | D-GN/WH | 368 | Right Audio Signal (+) (U32)
B5 | TN/WH | 372 | Audio Common | B5 | TN/WH | 372 | Audio Common
B6 | BN/WH | 1571 | Traction Control Switch Signal | B6 | BN/WH | 1571 | Traction Control Switch Signal
B7 | GY | 8 | Instrument Panel Lamp Supply Voltage | B7 | GY | 8 | Instrument Panel Lamp Supply Voltage (NW7, NW9)
GY | 8 | Instrument Panel Lamp Supply Voltage (UK6)
B8-B9 | -- | -- | Not Used | B8-B9 | -- | -- | Not Used
B10 | BK | 1050 | Ground (NW7, NW9) | B10 | BK | 1050 | Ground (NW7, NW9)
B11 | D-GN | 5060 | Low Speed GMLAN Serial Data | B11 | D-GN | 5060 | Low Speed GMLAN Serial Data
B12 | D-BU | 46 | Right Rear Speaker Output (+) | B12 | D-BU | 46 | Right Rear Speaker Output (+)
B13 | L-BU | 115 | Right Rear Speaker Output (-) | B13 | L-BU | 115 | Right Rear Speaker Output (-)
B14 | BN | 199 | Left Rear Speaker Output (+) | B14 | BN | 199 | Left Rear Speaker Output (+)
B15 | YE | 116 | Left Rear Speaker Output (-) | B15 | YE | 116 | Left Rear Speaker Output (-)

#### C300 Body Harness to Drivers Seat Harness

Connector Part Information

• | 15336205

• | 12-Way F GT Mixed Series (BK)

Connector Part Information

• | 15336209

• | 12-Way M GT Mixed Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/BK | 1242 | Battery Positive Voltage | A | RD/BK | 1242 | Battery Positive Voltage
B | D-GN | 5016 | Seat Belt Switch - Left - Signal | B | PK | 5016 | Seat Belt Switch - Left - Signal
C-E | -- | -- | Not Used | C-E | -- | -- | Not Used
F | BK | 1150 | Ground | F | BK | 1150 | Ground
BK | 1150 | Ground (2-Way Seat)
G | PK | 5057 | Low Reference | G | PK | 5057 | Low Reference
H | YE | 243 | Accessory Voltage (KA1) | H | YE | 243 | Accessory Voltage (KA1)
J | BK | 1140 | Battery Positive Voltage (KA1) (Sedan) | J | RD/WH | 1140 | Battery Positive Voltage (KA1)
RD/WH | 1140 | Battery Positive Voltage (KA1) (Extended Sedan)
K | GY | 8 | Instrument Panel Lamp Supply Voltage (KA1) | K | GY | 8 | Instrument Panel Lamp Supply Voltage (KA1)
L | -- | -- | Not Used | L | -- | -- | Not Used
M | BK | 1150 | Ground (KA1) | M | BK | 1150 | Ground (KA1)
BK | 1150 | Ground (KA1)

#### C304 Body Harness to LF Pretensioner Jumper Harness

Connector Part Information

• | 12110505

• | 2-Way F Metri-Pack 150 Series (YE)

Connector Part Information

• | 12110500

• | 2-Way M Metri-Pack 150 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control | A | OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
B | TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control | B | TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control

#### C305 Body Harness to RF Pretensioner Jumper Harness

Connector Part Information

• | 12110505

• | 2-Way F Metri-Pack 150 Series (YE)

Connector Part Information

• | 12110500

• | 2-Way M Metri-Pack 150 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG | 2117 | Seat Belt Pretensioner - Right - Low Control | A | OG/BK | 2117 | Seat Belt Pretensioner - Right - Low Control
B | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control | B | TN/WH | 2116 | Seat Belt Pretensioner - Right - High Control

#### C310 Body Harness to Passenger Seat Harness

Connector Part Information

• | 15326886

• | 4-Way F GT 280 Series (BK)

Connector Part Information

• | 15326889

• | 4-Way M GT 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YE | 243 | Accessory Voltage | A | YE | 243 | Accessory Voltage
YE | 243 | Accessory Voltage
B | BK | 1140 | Battery Positive Voltage (Sedan) | B | RD/WH | 1140 | Battery Positive Voltage
RD/WH | 1140 | Battery Positive Voltage (Extended Sedan)
C | GY | 8 | Instrument Panel Lamp Supply Voltage | C | GY | 8 | Instrument Panel Lamp Supply Voltage
D | BK | 1150 | Ground | D | BK | 1150 | Ground
BK | 1150 | Ground

#### C315 Video Screen Harness to DVD Jumper Harness

Connector Part Information

• | 104257-7

• | 8-Way F AMP (BK)

Connector Part Information

• | 103653-7

• | 8-Way M AMP (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD | -- | Video 8V | 1 | RD | -- | Video 8V
2 | RD/BK | -- | Video Ground | 2 | RD/BK | -- | Video Ground
3 | BN | -- | Select 1 | 3 | BN | -- | Select 1
4 | BN/BK | -- | Select 2 | 4 | BN/BK | -- | Select 2
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | TN | -- | Bright Control | 6 | TN | -- | Bright Control
7 | GN/BK | -- | Video Ground | 7 | GN/BK | -- | Video Ground
8 | GN | -- | Video Signal | 8 | GN | -- | Video Signal

#### C319 Body Harness to Left Inflatable Restraint Side Impact Module Jumper Harness (AY1)

Connector Part Information

• | 12110505

• | 2-Way F Metri-Pack 150 Series (YE)

Connector Part Information

• | 12110500

• | 2-Way M Metri-Pack 150 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN | 2137 | Side Impact Module - LF High Control | A | WH | 2137 | Side Impact Module - LF High Control
B | YE/BK | 2138 | Side Impact Module - LF Low Control | B | D-GN | 2138 | Side Impact Module - LF Low Control

#### C320 Body Harness to Right Inflatable Restraint Side Impact Module Jumper Harness (AY1)

Connector Part Information

• | 12110505

• | 2-Way F Metri-Pack 150 Series (YE)

Connector Part Information

• | 12110500

• | 2-Way M Metri-Pack 150 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN/WH | 2135 | Side Impact Module - RF High Control | A | WH | 2135 | Side Impact Module - RF High Control
B | L-GN | 2136 | Side Impact Module - RF Low Control | B | D-GN | 2136 | Side Impact Module - RF Low Control

#### C403 Body Harness to Rear Wheel Speed Sensor Harness (JL9)

Connector Part Information

• | 15326815

• | 4-Way F GT 150 Series Sealed 4.0 (BK)

Connector Part Information

• | 15326820

• | 4-Way M GT 150 Series Sealed 4.0 (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 884 | Left Rear Wheel Speed Sensor Supply Voltage | A | TN | 884 | Left Rear Wheel Speed Sensor Supply Voltage
B | OG | 885 | Left Rear Wheel Speed Sensor Signal | B | OG | 885 | Left Rear Wheel Speed Sensor Signal
C | BN | 882 | Right Rear Wheel Speed Sensor Supply Voltage | C | BN | 882 | Right Rear Wheel Speed Sensor Supply Voltage
D | WH | 883 | Right Rear Wheel Speed Sensor Signal | D | WH | 883 | Right Rear Wheel Speed Sensor Signal

#### C404 Liftgate Harness to Body Harness (Extended Sedan)

Connector Part Information

• | 12064752

• | 6-Way F Metri-Pack 280 Series, Self Lock (BK)

Connector Part Information

• | 12064754

• | 6-Way M Metri-Pack 280 Series, Self Lock (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PU | 293 | Rear Defog Element Supply Voltage | A | PU | 293 | Rear Defog Element Supply Voltage
B | WH | 17 | Stop Lamp Supply Voltage | B | WH | 17 | Stop Lamp Supply Voltage
C | BK | 1350 | Ground | C | BK | 1350 | Ground
D | WH/BK | 1221 | Liftgate Release Switch Signal | D | WH/BK | 1221 | Liftgate Release Switch Signal
E | BK | 1350 | Ground | E | BK | 1350 | Ground
BK | 1350 | Ground
F | -- | -- | Not Used | F | -- | -- | Not Used

#### C413 Fuel Sender Harness to Body Harness

Connector Part Information

• | 15326842

• | 10-Way F GT 150 Series, Sealed (BK)

Connector Part Information

• | 15444071

• | 9-Way M GT 150 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 1540 | Battery Positive Voltage | A | RD/WH | 1540 | Battery Positive Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control | B | WH | 1310 | EVAP Canister Vent Solenoid Control
C | GY | 120 | Fuel Pump Supply Voltage | C | GY | 120 | Fuel Pump Supply Voltage
D | BK | 1250 | Ground | D | BK | 1250 | Ground
E | OG/BK | 1057 | Low Reference | E | OG/BK | 1057 | Low Reference
F | BK/WH | 651 | Low Reference | F | OG/BK | 1057 | Low Reference
G | PU | 1589 | Fuel Level Sensor Signal | G | PU | 1589 | Fuel Level Sensor Signal
H | D-GN | 890 | Fuel Tank Pressure Sensor Signal | H | D-GN | 890 | Fuel Tank Pressure Sensor Signal
J | GY | 705 | 5-Volt Reference | J | GY | 705 | 5-Volt Reference
K | -- | -- | Not Used | K | -- | -- | Not Available

#### C500 Body Harness to Left Front Door Harness

Connector Part Information

• | 15401211

• | 40-Way F GT Mixed Series (GY)

Connector Part Information

• | 15401208

• | 40-Way M GT 150, 280 Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | YE | 343 | Accessory Voltage | A2 | YE | 343 | Accessory Voltage
A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal | A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal
A4 | GY | 118 | Left Front Speaker Output (-) | A4 | GY | 118 | Left Front Speaker Output (-)
GY | 118 | Left Front Speaker Output (-) (UZ6)
A5 | TN | 201 | Left Front Speaker Output (+) | A5 | TN | 201 | Left Front Speaker Output (+)
TN | 201 | Left Front Speaker Output (+) (UZ6)
A6 | BK | 1250 | Ground | A6 | BK | 1250 | Ground
BK | 1250 | Ground
A7 | BK | 1150 | Ground | A7 | BK | 1150 | Ground
A8 | -- | -- | Not Used | A8 | -- | -- | Not Used
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BK | 1150 | Ground (DL8) | B2 | BK | 1150 | Ground (DL8)
B3 | WH | 682 | Door Lock Lock/Unlock Signal | B3 | WH | 682 | Door Lock Lock/Unlock Signal
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage | B4 | GY | 8 | Instrument Panel Lamp Supply Voltage
B5 | TN | 694 | Driver Door Lock Actuator Unlock Control | B5 | TN | 694 | Driver Door Lock Actuator Unlock Control
B6 | GY/BK | 295 | Door Lock Actuator Lock Control | B6 | GY | 295 | Door Lock Actuator Lock Control
B7 | GY/BK | 745 | Left Front Door Ajar Switch Signal | B7 | GY/BK | 745 | Left Front Door Ajar Switch Signal
B8 | GY | 8 | Instrument Panel Lamp Supply Voltage | B8 | GY | 8 | Instrument Panel Lamp Supply Voltage
B9 | PU | 1124 | Door Lock Key Switch Unlock Signal | B9 | PU | 1124 | Door Lock Key Switch Unlock Signal
B10 | YE | 2131 | Side Impact Sensing Module - Left - Voltage (AY1) | B10 | YE | 2131 | Side Impact Sensing Module - Left - Voltage (AY1)
B11 | WH | 2132 | Side Impact Sensing Module - Left - Signal (AY1) | B11 | WH | 2132 | Side Impact Sensing Module - Left - Signal (AY1)
B12 | L-GN | 1123 | Door Lock Key Switch Lock Signal | B12 | L-GN | 1123 | Door Lock Key Switch Lock Signal
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | WH | 606 | Left Mirror Heating Element Supply Voltage (DL8) | C2 | WH | 606 | Left Mirror Heating Element Supply Voltage (DL8)
C3 | RD/WH | 640 | Battery Positive Voltage | C3 | RD/WH | 640 | Battery Positive Voltage
C4 | BK | 1150 | Ground | C4 | BK | 1150 | Ground
C5 | GY | 8 | Instrument Panel Lamp Supply Voltage | C5 | GY | 8 | Instrument Panel Lamp Supply Voltage
C6 | OG/WH | 881 | Right Mirror Motor Right Control | C6 | OG/WH | 881 | Right Mirror Motor Right Control
C7 | PU/WH | 889 | Right Mirror Motor Down Control | C7 | PU/WH | 889 | Right Mirror Motor Down Control
C8 | GY | 90 | Right Mirror Motor Left Control | C8 | GY | 90 | Right Mirror Motor Left Control
C9 | BK | 1150 | Ground | C9 | BK | 1150 | Ground
C10 | BN/WH | 2091 | Trunk Release Switch Supply Voltage | C10 | BN/WH | 2091 | Trunk Release Switch Supply Voltage
C11-C12 | -- | -- | Not Used | C11-C12 | -- | -- | Not Used
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal | D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
D3 | TN | 167 | Power Window Master Switch Right Front Down Signal | D3 | TN | 167 | Power Window Master Switch Right Front Down Signal
D4 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | D4 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
D5 | PU | 169 | Power Window Master Switch Left Rear Down Signal | D5 | PU | 169 | Power Window Master Switch Left Rear Down Signal
D6 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | D6 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
D7 | PU | 171 | Power Window Master Switch Right Rear Down Signal | D7 | PU | 171 | Power Window Master Switch Right Rear Down Signal
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

#### C600 Body Harness to Right Front Door Harness

Connector Part Information

• | 15401211

• | 40-Way F GT Mixed Series (GY)

Connector Part Information

• | 15401208

• | 40-Way M GT Mixed Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | YE | 343 | Accessory Voltage | A2 | YE | 343 | Accessory Voltage
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | D-GN | 117 | Right Front Speaker Output (-) | A4 | D-GN | 117 | Right Front Speaker Output (-)
D-GN | 117 | Right Front Speaker Output (-) (UZ6)
A5 | L-GN | 200 | Right Front Speaker Output (+) | A5 | L-GN | 200 | Right Front Speaker Output (+)
L-GN | 200 | Right Front Speaker Output (+) (UZ6)
A6 | BK | 1250 | Ground | A6 | BK | 1250 | Ground
BK | 1250 | Ground
A7-A8 | -- | -- | Not Used | A7-A8 | -- | -- | Not Used
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BK | 1150 | Ground | B2 | BK | 1150 | Ground
B3 | WH | 682 | Door Lock Lock/Unlock Signal | B3 | WH | 682 | Door Lock Lock/Unlock Signal
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage | B4 | GY | 8 | Instrument Panel Lamp Supply Voltage
B5 | TN | 294 | Door Lock Actuator Unlock Control | B5 | TN | 294 | Door Lock Actuator Unlock Control
B6 | GY/BK | 295 | Door Lock Actuator Lock Control | B6 | GY | 295 | Door Lock Actuator Lock Control
B7 | TN/WH | 746 | Passenger Door Ajar Switch Signal | B7 | TN/WH | 746 | Passenger Door Ajar Switch Signal
B8-B9 | -- | -- | Not Used | B8-B9 | -- | -- | Not Used
B10 | TN | 2133 | Side Impact Sensing Module - Right - Voltage (AY1) | B10 | TN | 2133 | Side Impact Sensing Module - Right - Voltage (AY1)
B11 | D-GN | 2134 | Side Impact Sensing Module - Right - Signal (AY1) | B11 | D-GN | 2134 | Side Impact Sensing Module - Right - Signal (AY1)
B12 | -- | -- | Not Used | B12 | -- | -- | Not Used
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | GY | 90 | Right Mirror Motor Left Control | C2 | GY | 90 | Right Mirror Motor Left Control
C3-C5 | -- | -- | Not Used | C3-C5 | -- | -- | Not Used
C6 | OG/WH | 881 | Right Mirror Motor Right Control | C6 | OG/WH | 881 | Right Mirror Motor Right Control
C7 | WH | 606 | Right Mirror Heating Element Supply Voltage (DL8) | C7 | WH | 606 | Right Mirror Heating Element Supply Voltage (DL8)
C8 | PU/WH | 889 | Right Mirror Motor Down Control | C8 | PU/WH | 889 | Right Mirror Motor Down Control
C9-C12 | -- | -- | Not Used | C9-C12 | -- | -- | Not Used
D1-D3 | -- | -- | Not Used | D1-D3 | -- | -- | Not Used
D4 | L-BU | 166 | Power Window Master Switch Right Front Up Signal | D4 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
D5 | TN | 167 | Power Window Master Switch Right Front Down Signal | D5 | TN | 167 | Power Window Master Switch Right Front Down Signal
D6-D8 | -- | -- | Not Used | D6-D8 | -- | -- | Not Used

#### C651 Headliner Harness to Body Harness

Connector Part Information

• | 15332129

• | 2-Way F GT 150 Series (BK)

Connector Part Information

• | 15332130

• | 2-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BARE | 1489 | Drain Wire | A | BARE | 1489 | Drain Wire
B | GY | 655 | Cellular Microphone Signal | B | GY | 655 | Cellular Microphone Signal

#### C700 Body Harness to Left Rear Door Harness

Connector Part Information

• | 15336211

• | 14-Way F GT 150, 280 Series (BK)

Connector Part Information

• | 15412364 (Sedan) 15479759 (Extended Sedan)

• | 14-Way M GT 150, 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | A | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
B | L-BU/BK | 747 | Passenger Door Ajar Switch Signal | B | L-BU/BK | 747 | Passenger Door Ajar Switch Signal
C | GY | 295 | Door Lock Actuator Lock Control | C | GY | 295 | Door Lock Actuator Lock Control
D | TN | 294 | Door Lock Actuator Unlock Control | D | TN | 294 | Door Lock Actuator Unlock Control
E | YE | 116 | Left Rear Speaker Output (-) (Extended Sedan) | E | YE | 116 | Left Rear Speaker Output (-) (Extended Sedan)
F | BN | 199 | Left Rear Speaker Output (+) (Extended Sedan) | F | BN | 199 | Left Rear Speaker Output (+) (Extended Sedan)
G | PU | 169 | Power Window Master Switch Left Rear Down Signal | G | PU | 169 | Power Window Master Switch Left Rear Down Signal
H | D-BU | 1307 | Power Window Master Switch Lockout Signal | H | D-BU | 1307 | Power Window Master Switch Lockout Signal
J | BK | 1250 | Ground | J | BK | 1250 | Ground
K-P | -- | -- | Not Used | K-P | -- | -- | Not Used

#### C707 Rear Lamp Harness to Left Tail Lamp Harness

Connector Part Information

• | 12160482

• | 4-Way F Metri-Pack 150 Series, Sealed (BK)

Connector Part Information

• | 12160470

• | 4-Way M Metri-Pack 150 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 1550 | Ground | A | BK | 1550 | Ground
B | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | B | L-BU | 18 | Left Rear Stop/Turn Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | L-GN | 24 | Backup Lamp Supply Voltage | D | L-GN | 24 | Backup Lamp Supply Voltage

#### C800 Body Harness to Right Rear Door Harness

Connector Part Information

• | 15336211

• | 14-Way F GT 150, 280 Series (BK)

Connector Part Information

• | 15412364 (Sedan) 15479759 (Extended Sedan)

• | 14-Way M GT 150, 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | A | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
B | L-GN/BK | 748 | Passenger Door Ajar Switch Signal | B | L-GN/BK | 748 | Passenger Door Ajar Switch Signal
C | GY | 295 | Door Lock Actuator Lock Control | C | GY | 295 | Door Lock Actuator Lock Control
D | TN | 294 | Door Lock Actuator Unlock Control | D | TN | 294 | Door Lock Actuator Unlock Control
E | L-BU | 115 | Right Rear Speaker Output (-) (Extended Sedan) | E | L-BU | 115 | Right Rear Speaker Output (-) (Extended Sedan)
F | D-BU | 46 | Right Rear Speaker Output (+) (Extended Sedan) | F | D-BU | 46 | Right Rear Speaker Output (+) (Extended Sedan)
G | PU | 171 | Power Window Master Switch Right Rear Down Signal | G | PU | 171 | Power Window Master Switch Right Rear Down Signal
H | D-BU | 1307 | Power Window Master Switch Lockout Signal | H | D-BU | 1307 | Power Window Master Switch Lockout Signal
J | BK | 1250 | Ground | J | BK | 1250 | Ground
K-P | -- | -- | Not Used | K-P | -- | -- | Not Used

#### C807 Rear Lamp Harness to Right Tail Lamp Harness

Connector Part Information

• | 12160482

• | 4-Way F Metri-Pack 150 Series, Sealed (BK)

Connector Part Information

• | 12160470

• | 4-Way M Metri-Pack 150 Series, Sealed (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 1450 | Ground | A | BK | 1450 | Ground
B | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | B | L-BU | 19 | Right Rear Stop/Turn Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | L-GN | 24 | Backup Lamp Supply Voltage | D | L-GN | 24 | Backup Lamp Supply Voltage