Handle, Panel, Switch - Outboard Passenger Seat. Chevrolet Evaluator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications. Refer to Fastener Tightening Specifications (Link disabled for test).
1 | Clip, Passenger Seat Recliner Handle Spring
2 | Handle, Passenger Seat Recliner
3 | Screw, Passenger Seat Cushion Outer Finish Panel Tighten: to 2.5 N·m (22 lb in).
4 | Panel, Passenger Seat Cushion Outer Finish Tip: Slide the panel toward the rear of the vehicle. Remove the panel from the recliner end first.
5 | Switch, Passenger Seat Heater
6 | Bolt, Front Seat Belt Anchor Tighten: to 35 N·m (25 lb ft).
7 | Anchor, Front Seat Belt
8 | Cover, Passenger Seat Cushion Outer Close Out