Fastener Tightening Specifications. Chevrolet Evaluator 1985

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
EPS Motor to Steering Column Bolts | 9 N·m | 80 lb in
Inner Tie Rod to Steering Gear | 95 N·m | 70 lb ft
Intermediate Steering Shaft to Steering Gear Pinch Bolt | 49 N·m | 36 lb ft
Rear Transmission Mount to Transmission Bolt | 90 N·m | 66 lb ft
Steering Gear to Frame Bolts

- First Pass

70 N·m

52 lb ft

- Final Pass

+ 90°

Tie Rod Torque Prevailing Nut | 60 N·m | 44 lb ft