Power and Grounding Schematic Icons. Chevrolet Evaluator 1985

For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Resistance wire with a stainless steel core. Approximately 6.6 ohms of resistance per meter (21.7 Feet).
| Caution: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.