Power Door Systems Connector End Views. Chevrolet Evaluator 1985

For 1990-2009 cars

Table 1: | C700 Body Side
Table 2: | C800 Body Side
Table 3: | C500 Body Side
Table 4: | C600 Body Side
Table 5: | Door Latch Assembly -- LF
Table 6: | Outside Rearview Mirror -- Left
Table 7: | Rear Compartment Lid Release Switch
Table 8: | Speaker -- LF
Table 9: | Speaker -- LF Upper
Table 10: | Outside Rearview Mirror Switch
Table 11: | Window Motor -- LF
Table 12: | Window Switch -- Master C1
Table 13: | Inflatable Restraint Side Impact Sensor -- Left
Table 14: | C500 Door Side
Table 15: | Door Lock Switch -- Driver
Table 16: | Window Switch -- Master C2
Table 17: | Door Latch Assembly -- LR
Table 18: | Window Motor -- RR
Table 19: | Window Switch -- LR
Table 20: | C700 Door Side

#### C700 Body Side

Connector Part Information

• | 15336211

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)
B | L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
C | GY | 295 | Door Lock Actuator Lock Control (AU3)
D | TN | 294 | Door Lock Actuator Unlock Control (AU3)
E | YE | 116 | Left Rear Speaker Signal (-) (U32/UK6&UC6/UP0)
E | YE | 116 | Left Rear Speaker Signal (-) (UC6/UP0-U32/UK6)
F | BN | 199 | Left Rear Speaker (+) (U32/UK6&UC6/UP0)
F | BN | 199 | Left Rear Speaker (+) (UC6/UP0-U32/UK6)
G | PU | 169 | Power Window Master Switch Left Rear Down Signal (A31)
H | D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
J | BK | 1250 | Ground

#### C800 Body Side

Connector Part Information

• | 15336211

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A31)
B | L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
C | GY | 295 | Door Lock Actuator Lock Control (AU3)
D | TN | 294 | Door Lock Actuator Unlock Control (AU3)
E | L-BU | 115;DP; | Right Rear Speaker Signal (-)
E | L-BU | 115;DN; | Right Rear Speaker Signal (-) (UC6/UP0-U32/UK6)
F | D-BU | 46;DP; | Right Rear Speaker (+) (U32/UK6&UC6/UP0)
F | D-BU | 46;DN; | Right Rear Speaker (+) (UC6/UP0-U32/UK6)
G | PU | 171 | Power Window Master Switch Right Rear Down Signal (A31)
H | D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
J | BK | 1250 | Ground

#### C500 Body Side

Connector Part Information

• | 15401211

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A2 | D-GN | 591 | Ignition 1 Relay Control
A3 | RD/BK | 242 | Battery Positive Voltage
A4 | RD/BK | 442 | Battery Positive Voltage
B2 | RD/BK | 342 | Battery Positive Voltage
B3 | RD/BK | 542 | Battery Positive Voltage (JL9&NW7/NW9)
B3 | RD/BK | 542 | Battery Positive Voltage (JL9&NW7/NW9)
B4 | RD/BK | 142 | Battery Positive Voltage
B5 | RD/BK | 42 | Battery Positive Voltage

#### C600 Body Side

Connector Part Information

• | 15401211

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A2 | YE | 343 | Accessory Voltage (A31)
A4 | D-GN | 117 | Right Front Speaker Signal (-) (UC6/UP0)
A5 | L-GN | 200 | Right Front Speaker (+) (UC6/UP0)
A6 | BK | 1250 | Ground
B10 | TN | 2133 | Right Front Side Impact Sensing Module Supply Voltage (AY1)
B11 | D-GN | 2134 | Right Front Side Impact Sensing Module Signal (AY1)
B2 | BK | 1150 | Ground (A31)
B3 | WH | 682 | Door Lock Lock/Unlock Signal (AU3)
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage (A31)
B5 | TN | 294 | Door Lock Actuator Unlock Control (AU3)
B6 | GY/BK | 295 | Door Lock Actuator Lock Control (AU3)
B7 | TN/WH | 746 | Right Front Door Ajar Switch Signal
C2 | GY | 90 | Right Mirror Motor Left Control (D49/DG6)
C6 | OG/WH | 881 | Right Mirror Motor Right Control (D49/DG6)
C7 | WH | 606 | Left Mirror Heating Element Supply Voltage (C49/DG6)
C8 | PU/WH | 889 | Right Mirror Motor Down Control (D49/DG6)
D4 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
D5 | TN | 167 | Power Window Master Switch Right Front Down Signal (A31)

#### Door Latch Assembly -- LF

Connector Part Information

• | 10768367

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
2 | TN | 694 | Driver Door Lock Actuator Unlock Control (AU3)
3 | GY | 295 | Door Lock Actuator Lock Control (AU3)
4 | L-GN | 1123 | Door Lock Key Switch Lock Signal
6 | GY/BK | 745 | Left Front Door Ajar Switch Signal
8 | BK | 1250 | Ground
9 | PU | 1124 | Door Lock Key Switch Unlock Signal

#### Outside Rearview Mirror -- Left

Connector Part Information

• | 12045688

• | 8 Way - M - Metri-Pack 150 Series BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | WH | 81 | Left Mirror Motor Right Control (D49/DG6)
B | L-BU | 82 | Left Mirror Motor Left Control (D49/DG6)
C | L-GN | 89 | Left Mirror Motor Down Control (D49/DG6)
D | WH | 606 | Left Mirror Heating Element Supply Voltage (DG6&D49/DG6)
E | BK | 1150 | Ground (DG6&D49/DG6)

#### Rear Compartment Lid Release Switch

Connector Part Information

• | 12047785

• | 4 Way - F - Metri-Pack 150 Series BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BK | 1150 | Ground
C | BN/WH | 2091 | Trunk Release Switch Supply Voltage
D | GY | 8 | Instrument Panel Lamp Supply Voltage (1)

#### Speaker -- LF

Connector Part Information

• | 12052832

• | 2 Way - F - Metri-Pack 150 Series BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | GY | 118 | Left Front Speaker Signal (-) (UC6/UP0)
B | TN | 201 | Left Front Speaker (+) (UC6/UP0)

#### Speaker -- LF Upper

Connector Part Information

• | 12052833

• | 2 Way - M - Metri-Pack 150 Series BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | GY | 118 | Left Front Speaker Signal (-) (UZ6&UC6/UP0)
B | TN | 201 | Left Front Speaker (+) (UZ6&UC6/UP0)

#### Outside Rearview Mirror Switch

Connector Part Information

• | 12064769

• | 10 Way - F - Metri-Pack 150 Series NA

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
B | BK | 1150 | Ground (D49/DG6)
C | GY | 90 | Right Mirror Motor Left Control (D49/DG6)
D | WH | 81 | Left Mirror Motor Right Control (D49/DG6)
E | GY | 8 | Instrument Panel Lamp Supply Voltage (1) (D49/DG6)
F | L-GN | 89 | Left Mirror Motor Down Control (D49/DG6)
G | RD/WH | 640 | Battery Positive Voltage (D49/DG6)
H | L-BU | 82 | Left Mirror Motor Left Control (D49/DG6)
J | OG/WH | 881 | Right Mirror Motor Right Control (D49/DG6)
K | PU/WH | 889 | Right Mirror Motor Down Control (D49/DG6)

#### Window Motor -- LF

Connector Part Information

• | 12129487

• | 2 Way - F - Metri-Pack 280 Series Flexlock Sealed GY

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BN | 165 | Power Window Motor Left Front Down Control (A31)
B | D-BU | 164 | Power Window Motor Left Front Up Control (A31)

#### Window Switch -- Master C1

Connector Part Information

• | 15326900

• | 6 Way - F - GT 280 BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BN | 165 | Power Window Motor Left Front Down Control (A31)
B | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
C | TN | 167 | Power Window Master Switch Right Front Down Signal (A31)
E | D-BU | 164 | Power Window Motor Left Front Up Control (A31)
F | GY | 8 | Instrument Panel Lamp Supply Voltage (1) (A31)
F | GY | 8 | Instrument Panel Lamp Supply Voltage (1) (A31)

#### Inflatable Restraint Side Impact Sensor -- Left

Connector Part Information

• | 15356724

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | WH | 2132 | Left Front Side Impact Sensing Module Signal (AY1)
B | YE | 2131 | Left Front Side Impact Sensing Module Supply Voltage (AY1)

#### C500 Door Side

Connector Part Information

• | 15401208

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A2 | YE | 343 | Accessory Voltage (A31)
A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal
A4 | GY | 118 | Left Front Speaker Signal (-) (UZ6&UC6/UP0)
A4 | GY | 118 | Left Front Speaker Signal (-) (UC6/UP0)
A5 | TN | 201 | Left Front Speaker (+) (UC6/UP0)
A5 | TN | 201 | Left Front Speaker (+) (UZ6&UC6/UP0)
A6 | BK | 1250 | Ground(AU3)
A6 | BK | 1250 | Ground
A7 | BK | 1150 | Ground (A31)
B10 | YE | 2131 | Left Front Side Impact Sensing Module Supply Voltage (AY1)
B11 | WH | 2132 | Left Front Side Impact Sensing Module Signal (AY1)
B12 | L-GN | 1123 | Door Lock Key Switch Lock Signal
B2 | BK | 1150 | Ground (DG6&D49/DG6)
B3 | WH | 682 | Door Lock Lock/Unlock Signal (AU3)
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage (AU3)
B5 | TN | 694 | Driver Door Lock Actuator Unlock Control (AU3)
B6 | GY | 295 | Door Lock Actuator Lock Control (AU3)
B7 | GY/BK | 745 | Left Front Door Ajar Switch Signal
B8 | GY | 8 | Instrument Panel Lamp Supply Voltage (1)
B9 | PU | 1124 | Door Lock Key Switch Unlock Signal
C10 | BN/WH | 2091 | Trunk Release Switch Supply Voltage
C2 | WH | 606 | Left Mirror Heating Element Supply Voltage (DG6&D49/DG6)
C3 | RD/WH | 640 | Battery Positive Voltage (D49/DG6)
C4 | BK | 1150 | Ground (D49/DG6)
C5 | GY | 8 | Instrument Panel Lamp Supply Voltage (D49/DG6)
C6 | OG/WH | 881 | Right Mirror Motor Right Control (D49/DG6)
C7 | PU/WH | 889 | Right Mirror Motor Down Control (D49/DG6)
C8 | GY | 90 | Right Mirror Motor Left Control (D49/DG6)
C9 | BK | 1150 | Ground
D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
D3 | TN | 167 | Power Window Master Switch Right Front Down Signal (A31)
D4 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)
D5 | PU | 169 | Power Window Master Switch Left Rear Down Signal
D6 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A31)
D7 | PU | 171 | Power Window Master Switch Right Rear Down Signal (A31)

#### Door Lock Switch -- Driver

Connector Part Information

• | 15417063

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BK | 1250 | Ground (AU3)
B | GY | 8 | Instrument Panel Lamp Supply Voltage (AU3)
C | WH | 682 | Door Lock Lock/Unlock Signal (AU3)

#### Window Switch -- Master C2

Connector Part Information

• | 15449340

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
B | BK | 1150 | Ground (A31)
C | PU | 169 | Power Window Master Switch Left Rear Down Signal (A31)
D | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)
E | YE | 343 | Accessory Voltage (A31)
F | D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
G | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A31)
H | PU | 171 | Power Window Master Switch Right Rear Down Signal (A31)

#### Door Latch Assembly -- LR

Connector Part Information

• | 10768369

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
2 | TN | 294 | Door Lock Actuator Unlock Control (AU3)
3 | GY | 295 | Door Lock Actuator Lock Control (AU3)
4 | L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
6 | BK | 1250 | Ground

#### Window Motor -- RR

Connector Part Information

• | 12129487

• | 2 Way - F - Metri-Pack 280 Series Flexlock Sealed GY

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BN | 669 | Power Window Motor Left Rear Down Control (A31)
B | D-BU | 668 | Power Window Motor Left Rear Up Control (A31)

#### Window Switch -- LR

Connector Part Information

• | 12191825

• | 8 Way - - Metri-Pack 280 Series BK

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
D | PU | 169 | Power Window Master Switch Left Rear Down Signal (A31)
F | BN | 669 | Power Window Motor Left Rear Down Control (A31)
G | D-BU | 668 | Power Window Motor Left Rear Up Control (A31)
H | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)

#### C700 Door Side

Connector Part Information

• | 15412364

• | ENTER PART DESCRIPTION HERE

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)
B | L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
C | GY | 295 | Door Lock Actuator Lock Control (AU3)
D | TN | 294 | Door Lock Actuator Unlock Control (AU3)
G | PU | 169 | Power Window Master Switch Left Rear Down Signal (A31)
H | D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
J | BK | 1250 | Ground