INFO - REDUCED RANGE/OPERATION OF RKE. Chevrolet Export Express 1999

For 1990-2009 cars

# INFO - REDUCED RANGE/OPERATION OF RKE

#### SUBJECT: INFORMATION - REDUCED RANGE/OPERATION OF REMOTE KEYLESS ENTRY (RKE)

#### MODELS: 1997-99 CHEVROLET AND GMC G VAN, M/L, C/K (EXCLUDING GMT800) SUBURBAN AND UTILITY MODELS

WHEN SOME OWNERS OF THE ABOVE VEHICLES ACTIVATE THE REMOTE KEYLESS ENTRY (RKE), THERE MAY BE A REDUCED RANGE/OPERATION OF THEIR RKE TRANSMITTERS. THIS MAY BE ATTRIBUTED TO THE LOCATION OF THE KEYLESS RECEIVER IN THE VEHICLE.

ALSO, IN SOME CASES WHERE THE TRANSMITTER COMMANDS A DOUBLE PRESS OF A BUTTON (I.E. "ALL DOOR UNLOCK" OR "REAR UNLOCK/HATCH RELEASE"), IF THE OWNER PRESSES THE BUTTON TOO RAPIDLY IN SUCCESSION, THE DOORS MAY NOT UNLOCK.

BECAUSE OF THE "ROLLING CODE" SECURITY ALGORITHM, THE RECEIVER MAY REQUIRE UP TO 1/2 OF A SECOND BETWEEN BUTTON PRESSES. BECAUSE OF THIS, ADVISE THE OWNER TO PAUSE ABOUT ONE SECOND BETWEEN DOUBLE PRESSING A BUTTON.

ALSO, IF AN OWNER IS UNABLE TO UNLOCK THE DOORS USING THE TRANSMITTER WHEN APPROACHING THE VEHICLE FROM THE REAR, ADVISE THE OWNER TO HOLD THE TRANSMITTER HIGHER SO THAT THE SIGNAL PASSES THROUGH THE REAR GLASS. ALSO, APPROACHING THE VEHICLE FROM THE SIDE USING THE TRANSMITTER MAY HELP TO UNLOCK THE DOORS.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.