Remote Mirror Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Pry off the outside rearview mirror inside trim cover (3).
2. Remove the mirror adjusting lever mounting nuts (2).
3. Remove the outside rearview mirror cover from the outside rearview mirror.
4. Remove the screws (2).
5. Remove the outside rearview mirror (1).

### Installation Procedure

1. Install the outside rearview mirror with the screws.
2. Install the outside rearview mirror cover.
3. Install the mirror adjusting lever with the nuts.
4. Install the outside rearview inside trim covers.