Clutch Pedal Free Travel Adjustment. Chevrolet Joy 2008

For 1990-2009 cars

Important: During inspection, take care on sudden departure.

It is designed that there is no clutch pedal free travel.

Specifications
The pedal travel (a) specifications equals 100-110 mm (3.9-4.3 in).

After starting the engine, check if the clearance between the pedal and floor is within the specified range in the condition of idling, lifting, parking brake, and drawing out the clutch pedal.

Specifications
The clearance between the pedal and floor just before the clutch connection (b) equals 30-40 mm (1.2-1.6 in).