Disassembled Views. Chevrolet Joy 2008

For 1990-2009 cars

Figure 1:

#### Cylinder Head

(1) | Oil Filter Cap
(2) | Cylinder Head Cover
(3) | Valve Spring
(4) | Intake Rocker Arm Shaft
(5) | Exhaust Rocker Arm Shaft
(6) | Water Outlet Case
(7) | Camshaft
(8) | Rocker Arm
(9) | Cylinder Head Gasket
(10) | Cylinder Head
(11) | Rocker Arm
(12) | Intake Valve
(13) | Exhaust Valve

Figure 2:

#### Engine Block

(1) | Oil Level Gage Stick
(2) | Piston
(3) | Connecting Rod
(4) | Engine Block
(5) | Oil Filter
(6) | Flywheel
(7) | Crankshaft
(8) | Oil Pan
(9) | Oil Pump Strainer
(10) | Oil Pump Assembly

Figure 3:

#### Manifold and Air Flow System

(1) | Intake Manifold
(2) | Exhaust Gas Recirculation (EGR) Pipe
(3) | Exhaust Gas Recirculation (EGR) Valve
(4) | Throttle Body Assembly
(5) | Air Filter Assembly
(6) | Resonator
(7) | Snorkel
(8) | Oxygen Sensor
(9) | Exhaust Manifold
(10) | Exhaust Manifold Heat Shield

Figure 4:

#### Timing Belt and Engine Mount

(1) | Engine Mount Damping Block
(2) | Engine Mount Intermediate Bracket
(3) | Engine Mount Bracket
(4) | Transaxle Mount Bracket
(5) | Transaxle Mount Damping Block
(6) | Engine Mount Front Bracket
(7) | Engine Mount Front Damping Bush
(8) | Timing Belt
(9) | Timing Belt Tensioner
(10) | Crankshaft Gear
(11) | Timing Belt Upper Front Cover
(12) | Timing Belt Lower Front Cover
(13) | Crankshaft Pulley
(14) | Engine Mount Lower Bracket
(15) | Engine Mount Upper Bracket