Displays and Gages Connector End Views. Chevrolet Joy 2008

For 1990-2009 cars

Connector 1: | Clock/Trip Odometer Switch
Connector 2: | Driver Information Center (DIC) C1
Connector 3: | Driver Information Center (DIC) C2
Connector 4: | Instrument Panel Cluster
Connector 5: | Overspeed Buzzer Relay (LHD)

### Clock/Trip Odometer Switch

#### Connector Part Information

- OEM: 5557-06R
- Service: N/A
- Description: 6-Way F Mini Fit (NA)

#### Clock/Trip Odometer Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 2133 | Clock Munite Reset
2 | WH | 2132 | Clock Hour Reset
3 | BK | 650 | Ground
4 | D-GN | 2134 | Clock Second Reset
5 | YE | 2131 | Odometer Reset
6 | -- | -- | Not Used

### Driver Information Center (DIC) C1

#### Connector Part Information

- OEM: KM01-12DS-HU(A)
- Service: N/A
- Description: 12-Way F 12 DS Series (BK)

#### Driver Information Center (DIC) C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
K1 | D-GN | 2386 | Odometer Off Voltage
K2 | D-BU | 15 | Right Turn Signal Lamp
K3 | L-GN | 62 | Hazard Indicator Control
K4 | BK | 550 | Ground
K5 | D-GN/YE | 35 | Coolant Temperature Indicator Control
K6 | PK | 39 | Ignition 1 Voltage
K7 | RD | 1340 | Battery Positive Voltage
K8 | YE | 804 | Door Open Signal
K9 | BN | 31 | Engine Oil IndicatorControl
K10 | L-GN | 11 | High Beam Indicator Control
K11 | YE/D-GN | 172 | Low Fuel Indicator Control
K12 | PK | 1561 | A/T Lamp Control

### Driver Information Center (DIC) C2

#### Connector Part Information

- OEM: KM01-12DS-HU(B)
- Service: N/A
- Description: 12-Way F 12DS Series (WH)

#### Driver Information Center (DIC) C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
K1 | L-GN | 867 | ABS Indicator Control
K2 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
K3-K4 | -- | -- | Not Used
K5 | BN/WH | 33 | Brake Warning Indicator Control
K6 | BN/YE | 25 | Charge Indicator Control
K7 | YE | 234 | Seat Belt Indicator Control
K8 | BN | 358 | Air Bag Indicator Control
K9 | OG | 122 | Rear Fog Lamp Voltage
K10 | BK | 550 | Ground
K11 | YE | 317 | Fog Lamps Voltage
K12 | L-BU | 14 | Left Turn Signal Lamp

### Instrument Panel Cluster

#### Connector Part Information

- OEM: 1123379-1
- Service: N/A
- Description: 20-Way F 040 Multilock Series Sealed (NA)

#### Instrument Panel Cluster

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 135 | Engine Temperature Gage Control
2 | YE | 2131 | Odometer Reset
3 | WH | 2132 | Clock Hour Reset
4 | BN | 2133 | Clock Minute Reset
5 | D-GN | 2134 | Clock Second Reset
6 | D-GN/GY | 264 | Security Indicator
7 | BN/WH | 309 | Illumination Voltage
8 | RD | 1340 | Battery Positive Voltage
9 | BK | 650 | Ground
10-12 | -- | -- | Not Used
13 | PU | 30 | Fuel Gage Control
14 | WH | 121 | Tachometer Signal
15 | BN/D-GN | 437 | Vehicle Speed Signal
16 | GY | 35 | Coolant Temperature Indicator Control
17 | -- | -- | Not Used
18 | YE/D-BU | 983 | Overspeed Buzzer
19 | D-GN | 44 | Illumination Ground
20 | PK | 39 | Ignition 1 Voltage

### Overspeed Buzzer Relay (LHD)

#### Connector Part Information

- OEM: AK36905
- Service: N/A
- Description: 9-Way F (BU)

#### Overspeed Buzzer Relay (LHD)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK/D-BU | 239 | Ignition 1 voltage
2 | YE/D-BU | 983 | Overspeed Warning Signal
3 | BK | 550 | Ground
4-9 | -- | -- | Not Used