General Specifications. Chevrolet Joy 2008

For 1990-2009 cars

## General Specifications 0.8L

Application | Specification
--- | ---
Metric | English
Clutch Disc

- Single Dry Plate

--

--

- Outside Diameter - Standard

170 mm

6.7 in

- Inside Diameter - Standard

110 mm

4.3 in

- Thickness - Standard

7.15 mm

0.281 in

- Rivet Head Depth - Limit

0.5 mm

0.02 in

- Rivet Head Depth - Standard

1.2 mm

0.047 in

- Disc Runout Limit in Rotational Direction - Limit

0.7 mm

0.028 in

Clutch Pedal

- Pedal Free Travel - Standard

0 mm

0 in

- Pedal Travel - Standard

100-110 mm

3.9-4.3 in

- Clearance between pedal and floor just before clutch connection - Limit

30-40 mm

1.2-1.6 in

## General Specifications 1.0L

Application | Specification
--- | ---
Metric | English
Clutch Disc

- Single Dry Plate

--

--

- Outside Diameter - Standard

184 mm

7.2 in

- Inside Diameter - Standard

127 mm

5.0 in

- Thickness - Standard

7.65 mm

0.301 in

- Rivet Head Depth - Standard

1.2 mm

0.047 in

- Rivet Head Depth - Limit

0.5 mm

0.020 in

- Disc Runout Limit in Rotational Direction - Limit

0.7 mm

0.028 in

Clutch Pedal

- Pedal Free Travel - Standard

0 mm

0 in

- Pedal Travel - Standard

105-115 mm

4.1-4.5 in

- Clearance between pedal and floor just before clutch connection - Limit

30-40 mm

1.2-1.6 in