Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Front Speed Sensor Retaining Bolt | 23 N·m | 17 lb ft
Control Arm Ball Stud Bolt | 60 N·m | 44 lb ft
Control Arm Mounting Bolt | 63 N·m | 47 lb ft
Crossmember Bolt | 22 N·m | 16 lb ft
Drive Axle-to-Hub Caulking Nut | 210 N·m | 155 lb ft
Front Under Longitudinal Frame Bolts | 70 N·m | 52 lb ft
Stabilizer Shaft Castellated Nut | 45 N·m | 33 lb ft
Stabilizer Shaft Mounting Nut and Bolt | 40 N·m | 30 lb ft
Strut Assembly-to-Body Nuts | 23 N·m | 17 lb ft
Strut Assembly-to-Knuckle Bolts | 80 N·m | 59 lb ft
Strut Closure Nut | 55 N·m | 41 lb ft
Tie Rod End-to-Knuckle Castellated Nut | 42 N·m | 31 lb ft
Wheel Hub-to-Brake Disc Bolt | 65 N·m | 48 lb ft