Theft Deterrent System Connector End Views. Chevrolet Joy 2008

For 1990-2009 cars

Connector 1: | Hood Open Switch
Connector 2: | Liftgate Ajar Switch
Connector 3: | Remote Control Door Lock Receiver (RCDLR)/Theft Deterrent Control Module
Connector 4: | Theft Deterrent Siren

### Hood Open Switch

#### Connector Part Information

- OEM: MG610392
- Service: N/A
- Description: 2-Way F SDL Series (WH)

#### Hood Open Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 40 | Battery Positive Voltage
2 | PK/BK | 109 | Hood Ajar Switch Signal

### Liftgate Ajar Switch

#### Connector Part Information

- OEM: MG610089
- Service: N/A
- Description: 1-Way F

#### Liftgate Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 804 | Rear Compartment Lid Ajar Switch Signal

### Remote Control Door Lock Receiver (RCDLR)/Theft Deterrent Control Module

#### Connector Part Information

- OEM: MG611336
- Service: N/A
- Description: 26-Way F PCB Series (WH)

#### Remote Control Door Lock Receiver (RCDLR)/Theft Deterrent Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 194 | Drive Door Unlock Control (AU0)
YE | 261 | Arm Alarm Signal (UA5)
2 | L-BU | 195 | Driver Door Lock Control (AU0)
BK | 550 | Ground (UA5)
3-4 | -- | -- | Not Used
5 | PK | 39 | Ignition 1 Voltage
6-7 | -- | -- | Not Used
8 | YE | 804 | Door Switch Signal
9-10 | -- | -- | Not Used
11 | RD/D-BU | 1140 | Battery Positive Voltage
12 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
13 | -- | -- | Not Used
14 | YE | 261 | Arm Alarm Signal (AU0)
15-16 | -- | -- | Not Used
17 | YE | 1398 | Immobilizer/Remote Keyless Entry Serial Data
18 | -- | -- | Not Used
19 | D-GN/GY | 264 | Security Indicator Voltage
20 | PK/BK | 109 | Hood Ajar Switch
21 | YE/RD | 143 | Accessory Voltage
22-23 | -- | -- | Not Used
24 | BK | 550 | Ground (AU0)
25 | -- | -- | Not Used
26 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Theft Deterrent Siren

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Assembly (BK)

#### Theft Deterrent Siren

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 261 | Arm Alarm Signal
2 | RD/WH | 40 | Battery Positive Voltage