Instrument Panel Air Outlet Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel from the instrument panel. Refer to Instrument Panel Outer Trim Cover Replacement .
2. Remove the vent screws (2).
3. Remove the vents (1) from the instrument cluster trim panel.

### Installation Procedure

1. Install the vents to the instrument cluster trim panel with the screws.
2. Install the instrument cluster trim panel. Refer to Instrument Panel Outer Trim Cover Replacement .