Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Booster-to-Dash Panel Nuts | 16 N·m | 12 lb ft
Brake Pedal Bracket Mounting Bolts | 18-26 N·m | 13-20 lb ft
Brake Pedal Bracket Mounting Nuts | 18-26 N·m | 13-20 lb ft
Brake Pedal-to-Pedal Bracket Hex Bolt | 18 N·m | 13 lb ft
Brake Pipe Fittings | 16 N·m | 12 lb ft
Brake Pipe Fittings to Front Caliper | 16 N·m | 12 lb ft
Brake Pipe Fittings to Master Cylinder | 16 N·m | 12 lb ft
Brake Pipe Fittings to Proportioning Valve | 16 N·m | 12 lb ft
Brake Pipe Fittings to Rear Wheel Cylinder | 16 N·m | 12 lb ft
Fluid Reservoir Screw | 4 N·m | 35 lb ft
Front Brake Hose-to-Caliper Bolt | 25.5 N·m | 19.1 lb ft
Master Cylinder Attaching Nuts | 16 N·m | 12 lb ft
Proportioning Valve | 22 N·m | 16 lb ft
Stop Lamp Switch Mounting Bracket Bolts | 9-12 N·m | 80-106 lb in