Rear Side Door Window Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the glass run. Refer to Rear Side Door Window Channel Replacement .

Notice: When removing glass from the vehicle, apply tape to corners of glass and adjacent surfaces to help prevent paint damage.

2. Remove the glass bolts (2).
3. Remove the glass (1).

### Installation Procedure

1. Install the glass with the bolts.
2. Install the glass run. Refer to Rear Side Door Window Channel Replacement