Rear Seat Back Cushion Latch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back assembly. Refer to Rear Seat Back Replacement .
2. Remove the lock knob from the seat back by twisting it (1).
3. Remove the rear seat back cover from the seat back frame.
4. Remove the bolts (1).
5. Remove the lock (2) from the seat back frame.

### Installation Procedure

1. Install the lock to the seat back frame with the bolts.
2. Install the rear seat back cover to the seat back frame.
3. Install the lock knob to the seat back.
4. Install the rear seat back assembly. Refer to Rear Seat Back Replacement .