High or Low Oil Pressure. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
Malfunction of Lubrication System

- Inadequate oil viscosity

Replace with the specified one.

- Loosening of the oil pressure switch

Tighten the switch.

- Lack of engine oil

Refill the oil.

- Blocking oil strainer

Clean the strainer.

- Lowered function of the oil pump

Replace the pump.

- Abrasion or damage of the oil pump relief valve

Replace the valve.