Front Disc Brake Pads Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Notice: Refer to Brake Caliper Notice in the Preface section.

1. Remove the front wheels. Refer to Tire and Wheel Removal and Installation .
2. Remove the brake pad pin bolt (1).
3. Lift the cylinder assembly (1).

Caution: Refer to Brake Dust Caution in the Preface section.

4. Remove the brake pads.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the brake pads and the cylinder assembly with the pin bolt (1).

Tighten
Tighten the pin bolt to 26 N·m (19 lb ft).

2. Install the front wheels. Refer to Tire and Wheel Removal and Installation .