Door Water Deflector Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .

Important: In case of the deluxe trim, remove the door pocket handle bracket in advance.

2. Remove the door seal trim (1).
3. Remove the door pocket handle bracket (2).

### Installation Procedure

1. Install the door seal trim.
2. Install the door pocket handle bracket for the deluxe trim.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .