Symptoms - Lighting Systems. Chevrolet Joy 2008

For 1990-2009 cars

Important: Review the system operation in order to familiarize yourself with the system functions.

Refer to Instrument Panel Description .

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the system. Refer to Checking Aftermarket Accessories.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing for Intermittent Conditions and Poor Connections.

### Symptom List

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom:

• | Backup Lamps Inoperative

• | Daytime Running Lamps (DRL) Inoperative

• | Fog Lamps Inoperative

• | Headlamps Inoperative - High Beams

• | Headlamps Inoperative - Low Beams

• | Low and High Beams Headlamps Inoperative

• | High Mount Stop Lamp Inoperative

• | Illuminated Entry Lamps Inoperative

• | Rear Compartment Lamp Inoperative

• | Stop Lamps Inoperative

• | Tail Lamps Inoperative

• | Turn Signal Lamps and/or Indicators Inoperative