Mirror Connector End Views. Chevrolet Joy 2008

For 1990-2009 cars

Connector 1: | Outside Rearview Mirror - Driver (DL6/Heated)
Connector 2: | Outside Rearview Mirror - Passenger (DL6/Heated)
Connector 3: | Outside Rearview Mirror - Passenger (DG2/DNB)
Connector 4: | Outside Rearview Mirror Switch

### Outside Rearview Mirror - Driver (DL6/Heated)

#### Connector Part Information

- OEM: MG651044
- Service: N/A
- Description: 6-Way F 090 II Series (NA)

#### Outside Rearview Mirror - Driver (DL6/Heated)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 650 | Ground
2 | -- | -- | Not Used
3 | RD/WH | 888 | Driver Mirror Motor Horizontal Control
4 | BN/WH | 330 | Mirror Motor Ground Control
5 | L-GN | 882 | Driver Mirror Motor Vertical Control
6 | OG | 267 | Mirror Heater Element Voltage

### Outside Rearview Mirror - Passenger (DL6/Heated)

#### Connector Part Information

- OEM: MG651044
- Service: N/A
- Description: 6-Way F 090 II Series (NA)

#### Outside Rearview Mirror - Passenger (DL6/Heated)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 650 | Ground
2 | -- | -- | Not Used
3 | L-GN | 889 | Passenger Mirror Motor Horizontal Control
4 | BN/WH | 330 | Mirror Motor Ground
5 | RD/WH | 881 | Passenger Mirror Motor Vertical Control
6 | OG | 267 | Mirror Heater Element Voltage

### Outside Rearview Mirror - Passenger (DG2/DNB)

#### Connector Part Information

- OEM: MG610394
- Service: N/A
- Description: 3-Way F SDL Series

#### Outside Rearview Mirror - Passenger (DG2/DNB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 330 | Mirror Motor Ground
2 | PU/WH | 889 | Mirror Motor Horizontal Control
3 | OG/WH | 881 | Passenger Mirror Motor Vertical Control

### Outside Rearview Mirror Switch

#### Connector Part Information

- OEM: 173850-1
- Service: N/A
- Description: 8-Way F Multilock 070 Series (WH)

#### Outside Rearview Mirror Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/WH | 881 | Passenger Mirror Motor Vertical Control (RHD, LHD w/DG2/DNB)
L-GN | 882 | Driver Mirror Motor Vertical Control (LHD w/DL6)
2 | -- | -- | Not Used
3 | OG/WH | 881 | Passenger Mirror Motor Vertical Control (LHD w/DL6)
L-GN | 882 | Driver Mirror Motor Vertical Control (RHD w/DL6)
4 | BN/WH | 330 | Mirror Motor Ground
5 | PU/WH | 889 | Passenger Mirror Motor Horizontal Control (RHD, LHD w/DG2/DNB)
RD/WH | 888 | Driver Mirror Motor Horizontal Control (LHD w/DL6)
6 | BK | 550 | Ground
7 | RD/WH | 888 | Driver Mirror Motor Horizontal Control (RHD w/DL6)
PU/WH | 889 | Passenger Mirror Motor Horizontal Control (LHD w/DL6)
8 | BN/YE | 141 | Ignition 2 Voltage