Rear Brake Backing Plate Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the brake drum. Refer to Brake Drum Replacement .
2. Remove the brake shoe components. Refer to Brake Shoe Replacement .
3. Remove the wheel cylinder assembly. Refer to Wheel Cylinder Replacement .
4. Remove the bolts and the backing plate.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the bolts and the backing plate (1).

Tighten
Tighten the backing plate-to-rear axle bolts to 24 N·m (18 lb ft).

2. Install the wheel cylinder assembly. Refer to Wheel Cylinder Replacement .
3. Install the brake shoe components. Refer to Brake Shoe Replacement .
4. Install the brake drum. Refer to Brake Drum Replacement .