Window Systems Component Views. Chevrolet Joy 2008

For 1990-2009 cars

Figure 1:

#### Front Door

(1) | Seal Trim
(2) | Lock Button
(3) | Trim Panel
(4) | Pocket Handle - Deluxe Type
(5) | Pocket Handle Bracket Deluxe Type - Deluxe Type
(6) | Inside Handle
(7) | Manual Regulator Handle
(8) | Pocket Handle - Standard Type
(9) | Door Speaker Cover
(10) | Map Pocket
(11) | Door Ajar Switch (Left Shown, Right Similar)
(12) | Striker
(13) | Opening Weatherstrip
(14) | Door Weatherstrip
(15) | Glass Run
(16) | Front Door
(17) | Inside Channel Weatherstrip
(18) | Inside Handle Rod
(19) | Door Latch (Left Shown, Right Similar)
(20) | Door Lock Cylinder Rod
(21) | Lock Rod
(22) | Actuator Rod
(23) | Actuator
(24) | Window Regulator and Motor (Driver Side Shown, Passenger Side Similar)
(25) | Outside Channel Weatherstrip
(26) | Outside Handle Rod
(27) | Outside Handle
(28) | Division Bar
(29) | Quarter Glass
(30) | Quarter Glass Run
(31) | Door Hinge
(32) | Door Hold Open Link
(33) | Power Window Switch Cover
(34) | Door Lock Actuator - Driver
(35) | Window Switch (Driver Side Shown, Passenger Side Similar)
(36) | Door Lock Actuator - Driver Blank
(37) | Door Side Molding

Figure 2:

#### Rear Door

(1) | Seal Trim
(2) | Lock Button
(3) | Trim Panel
(4) | Pocket Handle - Deluxe Type
(5) | Pocket Handle Bracket - Deluxe Type
(6) | Inside Handle
(7) | Manual Regulator Handle
(8) | Pocket Handle - Standard Type
(9) | Striker
(10) | Opening Weatherstrip
(11) | Door Weatherstrip
(12) | Glass Run
(13) | Interior Garnish Molding
(14) | Rear Door
(15) | Inside Channel Weatherstrip
(16) | Upper Guide Rail
(17) | Exterior Garnish Molding
(18) | Lower Guide Rail
(19) | Lock Rod
(20) | Door Latch (Left Shown, Right Similar)
(21) | Inside Handle Rod
(22) | Actuator Rod
(23) | Actuator (Lock) (Left Rear Shown, Right Similar)
(24) | Outside Handle Rod
(25) | Outside Handle
(26) | Window Regulator
(27) | Outside Channel Weatherstrip
(28) | Door Hinge
(29) | Door Hold Open Link
(30) | Door Side Molding