Clutch Vibration. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
Clutch facing with oily contamination | Replace the clutch disc.
Release bearing slides unsmoothly on input shaft bearing retainer | Lubricate the retainer release bearing.
Wobbly clutch disc or poor facing contact | Replace the clutch disc.
Loose clutch disc rivets | Replace the clutch disc.
Weakened clutch disc torsion spring | Replace the clutch disc.
Distorted pressure plate or flywheel surface | Replace the pressure plate or flywheel.
Weakened engine mounting or loosened installing bolt or nut | Retighten or replace the mounting.