Inline Harness Connector End Views. Chevrolet Joy 2008

For 1990-2009 cars

Connector 1: | C105 Engine Harness to Injector Harness
Connector 2: | C201 Floor Harness to I/P Harness
Connector 3: | C202 Engine Harness to I/P Harness (0.8L LHD)
Connector 4: | C202 I/P Harness to Engine Harness (0.8L RHD)
Connector 5: | C202 Engine Harness to I/P Harness (1.0L M/T LHD)
Connector 6: | C202 Engine Harness to I/P Harness (1.0L M/T RHD)
Connector 7: | C203 I/P Harness to Air Bag Harness
Connector 8: | C204 Front Harness to I/P Harness (LHD)
Connector 9: | C204 Front Harness to I/P Harness (RHD)
Connector 10: | C208 Roof Harness to I/P Harness
Connector 11: | C301 Floor Harness to Front Harness
Connector 12: | C351 I/P Harness to Driver Front Door Harness
Connector 13: | C352 Floor Harness to Driver Front Door Harness
Connector 14: | C361 I/P Harness to Passenger Front Door Harness
Connector 15: | C371 Floor Harness to Left Rear Door Harness (w/o Rear Power Windows)
Connector 16: | C371 Floor Harness to Left Rear Door Harness (w/Rear Power Windows)
Connector 17: | C381 Floor Harness to Right Rear Door Harness (w/o Rear Power Windows)
Connector 18: | C381 Floor Harness to Right Rear Door Harness (w/Rear Power Windows)
Connector 19: | C401 Liftgate Harness to Floor Harness

### C105 Engine Harness to Injector Harness

#### Connector Part Information

- OEM: MG610339-5
- Service: N/A
- Description: 8-Way F 070 SWP Series (BK)

#### Connector Part Information

- OEM: MG640341
- Service: N/A
- Description: 8-Way M (BK)

#### C105 Engine Harness to Injector Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | OG/BK | 1733 | Main Voltage Relay | 2 | OG/BK | 1733 | Main Voltage Relay
3-4 | -- | -- | Not Used | 3-4 | -- | -- | Not Used
5 | L-BU/BK | 844 | Fuel Injector 4 Control | 5 | L-BU/BK | 844 | Fuel Injector 4 Control
6 | PK/BK | 1746 | Fuel Injector 3 Control | 6 | PK/BK | 1746 | Fuel Injector 3 Control
7 | L-GN/BK | 1745 | Fuel Injector 2 Control | 7 | L-GN/BK | 1745 | Fuel Injector 2 Control
8 | BN | 1744 | Fuel Injector 1 Control | 8 | BN | 1744 | Fuel Injector 1 Control

### C201 Floor Harness to I/P Harness

#### Connector Part Information

- OEM: 936098-1
- Service: N/A
- Description: 26-Way F 090 III Series (NA)

#### Connector Part Information

- OEM: 936133-1
- Service: N/A
- Description: 26-Way M 090 III Series (NA)

#### C201 Floor Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | OG | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamp) | 1 | OG | 122 | Rear Fog Lamp Supply Voltage
2 | GY/YE | 596 | 5-Volt Reference | 2 | GY/YE | 596 | 5-Volt Reference
3 | L-BU | 14 | Left Turn Signal Voltage | 3 | L-BU | 14 | Left Turn Signal Voltage
4 | PU | 709 | Left Park Lamp Supply Voltage | 4 | PU | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage (w/Datyime Running Lights)
5 | L-BU/D-BU | 20 | Stop Lamp Supply Voltage | 5 | L-BU/D-BU | 20 | Stop Lamp Supply Voltage
L-BU/D-BU | 20 | Stop Lamp Supply Voltage | L-BU/D-BU | 20 | Stop Lamp Supply Voltage
6 | RD/WH | 840 | Battery Positive Voltage | 6 | RD/WH | 840 | Battery Positive Voltage
RD/WH | 840 | Battery Positive Voltage (LHD)
7 | GY/BK | 745 | Left Front Door Switch Signal | 7 | GY/BK | 745 | Left Front Door Switch Signal
8 | BN | 294 | Door Lock Actuator Unlock Control (w/Power Door Locks) | 8 | BN | 294 | Door Lock Actuator Unlock Control
BN | 294 | Door Lock Actuator Unlock Control
9 | YE | 234 | Seat Belt Indicator Control | 9 | YE | 234 | Seat Belt Indicator Control
10 | BN/YE | 141 | Ignition 2 Voltage | 10 | BN/YE | 141 | Ignition 2 Voltage (w/Rear Wiper and Washer)
11 | PU | 293 | Rear Defogger Voltage | 11 | PU | 293 | Rear Defogger Voltage (w/Rear Defogger)
12 | D-BU/WH | 46 | Right Rear Speaker Output (+) | 12 | D-BU/WH | 46 | Right Rear Speaker Output (+)
13 | YE/D-BU | 116 | Left Rear Speaker Output (-) | 13 | YE/D-BU | 116 | Left Rear Speaker Output (-)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | GY | 720 | Fuel Sender Low Reference | 15 | GY | 720 | Fuel Sender Low Reference
16 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 16 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
17 | BN/WH | 309 | Illumination Voltage | 17 | BN/WH | 309 | Illumination Voltage
BN/WH | 309 | Illumination Voltage
18 | L-GN | 24 | Back-Up Lamp Voltage | 18 | L-GN | 24 | Back-Up Lamp Voltage
19 | YE/D-GN | 172 | Low Fuel Indicator Control | 19 | YE/D-GN | 172 | Low Fuel Indicator Control
20 | YE | 804 | Door Switch Signal | 20 | YE | 804 | Door Switch Signal
YE | 804 | Door Switch Signal (LHD)
21 | GY | 295 | Door Lock Actuator Lock Control (w/Power Door Locks) | 21 | GY | 295 | Door Lock Actuator Lock Control
GY | 295 | Door Lock Actuator Lock Control
22 | BN/WH | 33 | Brake Indicator Control | 22 | BN/WH | 33 | Brake Indicator Control (LHD)
BN | 33 | Brake Indicator Control (RHD)
23 | GY/WH | 391 | Rear Wiper Switch Signal | 23 | GY/WH | 391 | Rear Wiper Switch Signal (w/Rear Wiper and Washer)
24 | GY/BK | 120 | Fuel Pump Supply Voltage | 24 | GY/BK | 120 | Fuel Pump Supply Voltage
25 | L-BU/RD | 115 | Right Rear Speaker Output (-) | 25 | L-BU/RD | 115 | Right Rear Speaker Output (-)
26 | BN/YE | 199 | Left Rear Speaker Output (+) | 26 | BN/YE | 199 | Left Rear Speaker Output (+)

### C202 Engine Harness to I/P Harness (0.8L LHD)

#### Connector Part Information

- OEM: MG611133
- Service: N/A
- Description: 22-Way F .2507 Series (NA)

#### Connector Part Information

- OEM: MG621134
- Service: N/A
- Description: 22-Way M .2507 Series (NA)

#### C202 Engine Harness to I/P Harness (0.8L LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | PK | 1561 | Automatic Transmission Warning Lamp Signal (A/T) | 2 | PK | 1561 | Automatic Transmission Warning Lamp Signal (A/T)
3 | D-GN | 2386 | Overdrive Off Switch (A/T) | 3 | D-GN | 2386 | Overdrive Off Switch (A/T)
4 | PU | 1319 | Serial Data | 4 | PU | 1319 | Serial Data (w/o Theft)
L-GN | 488 | Power Take-Off Enable Switch (w/Theft)
5 | D-GN/WH | 762 | A/C Request Signal | 5 | D-GN/WH | 762 | A/C Request Signal (C60/C68)
6 | D-BU | 732 | Evaporator Temperature Signal | 6 | D-BU | 732 | Evaporator Temperature Signal (C60/C68)
7 | BN/D-BU | 718 | Low Reference | 7 | BN/D-BU | 718 | Low Reference (C60/C68)
BN/D-BU | 718 | Low Reference (M/T)
8 | GY/YE | 596 | Fuel Sender Signal | 8 | GY/YE | 596 | Fuel Sender Signal
9 | GY/BK | 720 | Sensor Ground | 9 | GY | 720 | Sensor Ground
10 | PU | 30 | Fuel Gage Signal | 10 | PU | 30 | Fuel Gage Signal
11 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control | 11 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
12 | BN/D-GN | 437 | Vehicle Speed Sensor Signal (A/T) | 12 | YE | 400 | Vehicle Speed Sensor Signal
BN/D-GN | 437 | Vehicle Speed Sensor Signal (M/T)
BN/D-GN | 437 | Vehicle Speed Sensor Signal (M/T)
13 | WH | 121 | Tachometer Signal | 13 | WH | 121 | Tachometer Signal
14 | D-GN/WH | 135 | Temperature Signal | 14 | D-GN/WH | 135 | Temperature Signal
15 | BN/BK | 241 | Ignition 2 Voltage | 15 | BN/BK | 241 | Ignition 2 Voltage
16 | L-GN | 24 | Back-Up Lamp Voltage (A/T) | 16 | L-GN | 24 | Back-Up Lamp Voltage
L-GN | 24 | Back-Up Lamp Voltage
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | GY/BK | 2387 | Serial Data (A/T) | 18 | GY/BK | 2387 | Serial Data (A/T)
19 | YE | 5 | Starter Solenoid (A/T) | 19 | PU/RD | 5 | Starter Solenoid
PU | 6 | Starter Solenoid (M/T)
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | BN | 31 | Oil Pressure Indicator Lamp | 21 | BN | 31 | Oil Pressure Indicator Lamp
BN | 31 | Oil Pressure Indicator Lamp (w/Daytime Running Lights)
22 | BN/YE | 25 | Charge Indicator Lamp | 22 | BN/YE | 25 | Charge Indicator Lamp

### C202 I/P Harness to Engine Harness (0.8L RHD)

#### Connector Part Information

- OEM: 936151-1
- Service: N/A
- Description: 22-Way F 090 III Series (NA)

#### Connector Part Information

- OEM: 936154-1
- Service: N/A
- Description: 22-Way M 090 III Series (NA)

#### C202 I/P Harness to Engine Harness (0.8L RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU/RD | 5 | Starter Solenoid | 1 | YE | 5 | Starter Solenoid
2 | D-GN | 2386 | Overdrive Off Switch (A/T) | 2 | D-GN | 2386 | Overdrive Off Switch (A/T)
D-GN | 2386 | Overdrive Off Switch (A/T)
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | PK | 1561 | A/T Warning Lamp Signal (A/T) | 4 | PK | 1561 | A/T Warning Lamp Signal (A/T)
5 | L-GN | 24 | Back-Up Lamp Voltage | 5 | L-GN | 24 | Back-Up Lamp Voltage
6 | D-GN/WH | 762 | A/C Request Signal (C60/C68) | 6 | D-GN/WH | 762 | A/C Request Signal
7 | BN/D-BU | 718 | Low Reference (C60/C68) | 7 | BN/D-BU | 718 | Low Reference
8 | BN | 31 | Oil Pressure Indicator Lamp | 8 | BN | 31 | Oil Pressure Indicator Lamp
9 | BN/WH | 419 | Check Engine Indicator Lamp | 9 | BN/WH | 419 | Check Engine Indicator Lamp
10 | D-GN/WH | 135 | Temperature Signal | 10 | D-GN/WH | 135 | Temperature Signal
11 | WH | 121 | Tachometer Signal | 11 | WH | 121 | Tachometer Signal
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | BN/BK | 241 | Ignition 2 Voltage | 13 | BN/BK | 241 | Ignition 2 Voltage
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | GY/BK | 2387 | Serial Data (A/T) | 15 | GY/BK | 2387 | Serial Data (A/T)
16 | PU | 1319 | Serial Data (w/o Theft) | 16 | PU | 1319 | Serial Data
L-GN | 488 | Power Take-Off Enable Switch (w/Theft)
17 | BN/D-GN | 437 | Vehicle Speed Signal | 17 | YE | 400 | Vehicle Speed Sensor Signal (A/T)
BN/D-GN | 437 | Vehicle Speed Signal (M/T)
BN/D-GN | 437 | Vehicle Speed Signal (M/T)
18 | D-BU | 732 | Evaporator Temperature Signal (w/Air Conditioning) | 18 | D-BU | 732 | Evaporator Temperature Signal
19 | BN/YE | 25 | Charge Indicator Lamp | 19 | BN/YE | 25 | Charge Indicator Lamp
20 | GY/YE | 596 | Fuel Sender Signal | 20 | GY/YE | 596 | Fuel Sender Signal
21 | GY | 720 | Sensor Ground | 21 | GY | 720 | Sensor Ground
22 | PU | 30 | Fuel Gage Signal | 22 | PU | 30 | Fuel Gage Signal

### C202 Engine Harness to I/P Harness (1.0L M/T LHD)

#### Connector Part Information

- OEM: MG611133
- Service: N/A
- Description: 22-Way F .2507 Series (NA)

#### Connector Part Information

- OEM: MG6221134
- Service: N/A
- Description: 22-Way M .2507 Series (NA)

#### C202 Engine Harness to I/P Harness (1.0L M/T LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-3 | -- | -- | Not Used | 1-3 | -- | -- | Not Used
4 | PU | 1319 | Serial Data | 4 | PU | 1319 | Serial Data (w/o Theft)
L-GN | 488 | Power Take-Off Enable Switch (w/Theft)
5 | D-GN/WH | 762 | A/C request Signal | 5 | D-GN/WH | 762 | A/C Request Signal (C60/C68)
6 | D-BU | 732 | Evaporator Temperature Signal | 6 | D-BU | 732 | Evaporator Temperature Signal (C60/C68)
7 | BN/D-BU | 718 | Low Reference | 7 | BN/D-BU | 718 | Low Reference (C60/C68)
8 | GY/YE | 596 | Fuel Sender Signal | 8 | GY/YE | 596 | Fuel Sender Signal
9 | BN | 808 | Low Reference | 9 | GY | 720 | Sensor Ground
10 | PU | 30 | Fuel Gage Signal | 10 | PU | 30 | Fuel Gage Signal
11 | BN/WH | 419 | Check Engine Indicator Lamp | 11 | BN/WH | 419 | Check Engine Indicator Lamp
12 | BN/D-GN | 437 | Vehicle Speed Signal | 12 | BN/D-GN | 437 | Vehicle Speed Signal
BN/D-GN | 437 | Vehicle Speed Signal
13 | WH | 121 | Tachometer Signal | 13 | WH | 121 | Tachometer Signal
14 | D-GN/WH | 135 | Temperature Gage Signal | 14 | D-GN/WH | 135 | Temperature Gage Signal
15 | BN/BK | 241 | Ignition 2 Voltage | 15 | BN/BK | 241 | Ignition 2 Voltage
16 | L-GN | 24 | Back-Up Lamp Voltage | 16 | L-GN | 24 | Back-Up Lamp Voltage
17-18 | -- | -- | Not Used | 17-18 | -- | -- | Not Used
19 | PU | 6 | Starter Solenoid | 19 | PU/RD | 5 | Starter Solenoid
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | BN | 31 | Oil Pressure Indicator Lamp | 21 | BN | 31 | Oil Pressure Indicator Lamp
BN | 31 | Oil Pressure Indicator Lamp (w/Daytime Running Lights)
22 | BN/YE | 25 | Charge Indicator Lamp | 22 | BN/YE | 25 | Charge Indicator Lamp

### C202 Engine Harness to I/P Harness (1.0L M/T RHD)

#### Connector Part Information

- OEM: 936151-1
- Service: N/A
- Description: 22-Way F 090 III Series (NA)

#### Connector Part Information

- OEM: 936154-1
- Service: N/A
- Description: 22-Way M 090 III Series (NA)

#### C202 Engine Harness to I/P Harness (1.0L M/T RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU/RD | 5 | Starter Solenoid | 1 | PU | 6 | Starter Solenoid
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | L-GN | 24 | Back-Up Lamp Voltage | 5 | L-GN | 24 | Back-Up Lamp Voltage
6 | D-GN/WH | 762 | A/C request Signal (w/Air Conditioning) | 6 | D-GN/WH | 762 | A/C request Signal
7 | BN/D-BU | 718 | Low Reference (w/Air Conditioning) | 7 | D-GN/WH | 718 | Low Reference
8 | BN | 31 | Oil Pressure Indicator Lamp | 8 | BN | 31 | Oil Pressure Indicator Lamp
9 | BN/WH | 419 | Check Engine Indicator Lamp | 9 | BN/WH | 419 | Check Engine Indicator Lamp
10 | D-GN/WH | 135 | Temperature Gage Signal | 10 | D-GN/WH | 135 | Temperature Gage Signal
11 | WH | 121 | Tachometer Signal | 11 | WH | 121 | Tachometer Signal
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | BN/BK | 241 | Fuse Output - Ignition 3 | 13 | BN/BK | 241 | Fuse Output - Ignition 3
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | -- | -- | Not Used | 15 | -- | -- | Not Used
16 | L-GN | 488 | Power Take-Off Enable Switch (w/Theft) | 16 | PU | 1319 | Serial Data
PU | 1319 | Serial Data (w/o Theft)
17 | BN/D-GN | 437 | Vehicle Speed Signal | 17 | BN/D-GN | 437 | Vehicle Speed Signal
18 | D-BU | 732 | Evaporator Temperature Signal (w/Air Conditioning) | 18 | D-BU | 732 | Evaporator Temperature Signal
19 | BN/YE | 25 | Charge Indicator Lamp | 19 | BN/YE | 25 | Charge Indicator Lamp
20 | GY/YE | 596 | Fuel Sender Signal | 20 | GY/YE | 596 | Fuel Sender Signal
21 | GY | 720 | Sensor Ground | 21 | BN | 808 | Low Reference
22 | PU | 30 | Fuel Gage Signal | 22 | PU | 30 | Fuel Gage Signal

### C203 I/P Harness to Air Bag Harness

#### Connector Part Information

- OEM: 174928-1
- Service: N/A
- Description: 3-Way F .070 Multilock Series (WH)

#### Connector Part Information

- OEM: 368500-1
- Service: N/A
- Description: 3-Way M .070 Multilock Series (NA)

#### C203 I/P Harness to Air Bag Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PK/BK | 139 | Ignition 2 Voltage | 1 | PK/BK | 139 | Ignition 2 Voltage
2 | L-GN | 377 | SDM Serial Data | 2 | L-GN | 377 | SDM Serial Data
3 | BN | 358 | Air Bag Warning Lamp | 3 | BN | 358 | Air Bag Warning Lamp

### C204 Front Harness to I/P Harness (LHD)

#### Connector Part Information

- OEM: 936227-1
- Service: N/A
- Description: 4-Way F 090 II Series (NA)

#### Connector Part Information

- OEM: 936238-1
- Service: N/A
- Description: 4-Way M 090 II Series (NA)

#### C204 Front Harness to I/P Harness (LHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 261 | Arm Alarm Signal (w/Remote Keyless) | 1 | YE | 261 | Arm Alarm Signal
2 | PK/BK | 109 | Hood Ajar Switch Signal (w/Remote Keyless) | 2 | PK/BK | 109 | Hood Ajar Switch Signal
3 | -- | -- | Not Used | 3 | L-GN/BK | 735 | Outside Ambient Air Temperature Sensor High
4 | -- | -- | Not Used | 4 | YE | 61 | Outside Ambient Air Temperature Sensor Low

### C204 Front Harness to I/P Harness (RHD)

#### Connector Part Information

- OEM: 936268-1
- Service: N/A
- Description: 6-Way F 090 Series (NA)

#### Connector Part Information

- OEM: 936271-1
- Service: N/A
- Description: 6-Way M 090 Series (NA)

#### C204 Front Harness to I/P Harness (RHD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 261 | Arm Alarm Signal | 1 | YE | 261 | Arm Alarm Signal (CAL)
2 | BN | 41 | Ignition 2 Voltage | 2 | BN | 41 | Ignition 2 Voltage
3 | BN/WH | 96 | Wiper Motor Pulse Delay Signal | 3 | BN/WH | 96 | Wiper Motor Pulse Delay Signal
4 | PK/BK | 109 | Hood Ajar Switch Signal | 4 | PK/BK | 109 | Hood Ajar Switch Signal (CAL)
5 | D-GN/YE | 95 | Wiper Motor Low Speed | 5 | D-GN/YE | 95 | Wiper Motor Low Speed
6 | PU | 92 | Wiper Motor High Speed | 6 | PU | 92 | Wiper Motor High Speed

### C208 Roof Harness to I/P Harness

#### Connector Part Information

- OEM: 936224-1
- Service: N/A
- Description: 2-Way F 090 II Series (NA)

#### Connector Part Information

- OEM: 936236-1
- Service: N/A
- Description: 2-Way M 090 II Series (NA)

#### C208 Roof Harness to I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 804 | Door Switch Signal | 1 | YE | 804 | Door Switch Signal
2 | RD/WH | 840 | Battery Voltage | 2 | RD/WH | 840 | Battery Voltage

### C301 Floor Harness to Front Harness

#### Connector Part Information

- OEM: 936227-1
- Service: N/A
- Description: 4-Way F 090 II Series (NA)

#### Connector Part Information

- OEM: 936238-1
- Service: N/A
- Description: 4-Way M 090 II Series (NA)

#### C301 Floor Harness to Front Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | WH | 883 | Right Rear Wheel Speed Sensor Return | 1 | WH | 883 | Right Rear Wheel Speed Sensor Return
2 | BN | 882 | Right Rear Wheel Speed Sensor Signal | 2 | BN | 882 | Right Rear Wheel Speed Sensor Signal
3 | OG | 885 | Left Rear Wheel Speed Sensor Return | 3 | OG | 885 | Left Rear Wheel Speed Sensor Return
4 | BN | 884 | Left Rear Wheel Speed Sensor Signal | 4 | BN | 884 | Left Rear Wheel Speed Sensor Signal

### C351 I/P Harness to Driver Front Door Harness

#### Connector Part Information

- OEM: MG612231
- Service: N/A
- Description: 8-Way F ASC Series (NA)

#### Connector Part Information

- OEM: MG622232
- Service: N/A
- Description: 8-Way M 090 Series (NA)

#### C351 I/P Harness to Driver Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-BU | 166 | LH Power Window Motor Up | 1 | L-BU | 166 | LH Power Window Motor Up
2 | PK/WH | 539 | Ignition Voltage | 2 | PK/WH | 539 | Ignition Voltage
3 | BN | 294 | Power Door Lock Motor Unlock Feed (w/Power Door Locks) | 3 | BN | 294 | Power Door Lock Motor Unlock Feed (w/Power Door Locks)
4 | BN | 167 | RH Front Power Window Down | 4 | BN | 167 | RH Front Power Window Down
5 | D-BU | 1307 | Ignition Voltage (w/Rear Power Windows) | 5 | D-BU | 1307 | Ignition Voltage (w/Rear Power Windows)
6 | BK | 650 | Ground | 6 | BK | 550 | Ground
7 | RD/D-BU | 1140 | Ignition Voltage (Power Door Locks w/o CAL) | 7 | RD/D-BU | 1140 | Ignition Voltage (Power Door Locks)
YE | 356 | Power Door Lock Signal (CAL)
8 | GY | 295 | Power Door Lock Motor Lock Feed | 8 | GY | 295 | Power Door Lock Motor Lock Feed (w/Power Door Locks)
GY | 295 | Power Door Lock Motor Lock Feed (w/Power Door Locks)

### C352 Floor Harness to Driver Front Door Harness

#### Connector Part Information

- OEM: MG612228
- Service: N/A
- Description: 6-Way F ASC Series (NA)

#### Connector Part Information

- OEM: MG622229
- Service: N/A
- Description: 6-Way M ASC Series (NA)

#### C352 Floor Harness to Driver Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN | 170 | RH Rear Power Window Motor Up | 1 | L-GN | 170 | RH Rear Power Window Motor Up
2 | D-GN | 168 | LH Rear Power Window Motor Up | 2 | D-GN | 168 | LH Rear Power Window Motor Up
3 | PU | 171 | RH Rear Power Window Motor Down | 3 | PU | 171 | RH Rear Power Window Motor Down
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | D-BU | 1307 | Ignition 1 Voltage | 5 | D-BU | 1307 | Ignition 1 Voltage
6 | PU | 169 | LH Rear Power Window Motor Down | 6 | PU | 169 | LH Rear Power Window Motor Down

### C361 I/P Harness to Passenger Front Door Harness

#### Connector Part Information

- OEM: MG612231
- Service: N/A
- Description: 8-Way F ASC Series (NA)

#### Connector Part Information

- OEM: MG622232
- Service: N/A
- Description: 8-Way M 090 Series (NA)

#### C361 I/P Harness to Passenger Front Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 167 | Power Window Switch Down | 1 | BN | 167 | Power Window Switch Down
2 | D-BU | 1307 | Ignition Voltage (w/Rear Power Windows) | 2 | D-BU | 1307 | Ignition Voltage (w/Rear Power Windows)
PK/WH | 539 | Ignition Voltage (w/o Rear Power Windows) | PK/WH | 539 | Ignition Voltage (w/o Rear Power Windows)
3 | GY | 295 | Power Door Lock Feed (w/Power Door Locks) | 3 | GY | 295 | Power Door Lock Feed (w/Power Door Locks)
4 | L-BU | 166 | Power Window Switch Down | 4 | L-BU | 166 | Power Window Switch Down
5 | OG/WH | 881 | Power Mirror Motor Vertical (w/Power Mirror) | 5 | OG/WH | 881 | Power Mirror Motor Vertical (w/Power Mirror)
6 | BN/WH | 330 | Power Mirror Motor Ground (w/Power Mirror) | 6 | BN/WH | 330 | Power Mirror Motor Ground (w/Power Mirror)
7 | PU/WH | 889 | Power Mirror Motor Horizontal (w/Power Mirror) | 7 | PU/WH | 889 | Power Mirror Motor Horizontal (w/Power Mirror)
8 | BN | 294 | Power Door Lock Unlock Feed | 8 | BN | 294 | Power Door Lock Unlock Feed

### C371 Floor Harness to Left Rear Door Harness (w/o Rear Power Windows)

#### Connector Part Information

- OEM: MG611857
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Connector Part Information

- OEM: MG621858
- Service: N/A
- Description: 2-Way M ASC Series (NA)

#### C371 Floor Harness to Left Rear Door Harness (w/o Rear Power Windows)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 294 | Power Door Lock Motor Unlock | 1 | BN | 294 | Power Door Lock Motor Unlock
2 | GY | 295 | Power Door Lock Motor Lock | 2 | GY | 295 | Power Door Lock Motor Lock

### C371 Floor Harness to Left Rear Door Harness (w/Rear Power Windows)

#### Connector Part Information

- OEM: MG612228
- Service: N/A
- Description: 6-Way F ASC Series (NA)

#### Connector Part Information

- OEM: MG622229
- Service: N/A
- Description: 6-Way M ASC Series (NA)

#### C371 Floor Harness to Left Rear Door Harness (w/Rear Power Windows)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 294 | Power Door Lock Motor Unlock | 1 | BN | 294 | Power Door Lock Motor Unlock
2 | GY | 295 | Power Door Lock Motor Lock | 2 | GY | 294 | Power Door Lock Motor Lock
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | D-BU | 1307 | Ignition 1 Voltage | 4 | D-BU | 1307 | Ignition 1 Voltage
5 | PU | 169 | Power Window Switch Down | 5 | PU | 169 | Power Window Switch Down
6 | D-GN | 168 | Power Window Switch Up | 6 | D-GN | 168 | Power Window Switch Up

### C381 Floor Harness to Right Rear Door Harness (w/o Rear Power Windows)

#### Connector Part Information

- OEM: MG611857
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Connector Part Information

- OEM: MG621858
- Service: N/A
- Description: 2-Way M ASC Series (NA)

#### C381 Floor Harness to Right Rear Door Harness (w/o Rear Power Windows)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 294 | Power Door Lock Motor Unlock | 1 | BN | 294 | Power Door Lock Motor Unlock
2 | GY | 295 | Power Door Lock Motor Lock | 2 | GY | 294 | Power Door Lock Motor Lock

### C381 Floor Harness to Right Rear Door Harness (w/Rear Power Windows)

#### Connector Part Information

- OEM: MG612228
- Service: N/A
- Description: 6-Way F ASC Series (NA)

#### Connector Part Information

- OEM: MG622229
- Service: N/A
- Description: 6-Way M ASC Series (NA)

#### C381 Floor Harness to Right Rear Door Harness (w/Rear Power Windows)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 294 | Power Door Lock Motor Unlock | 1 | BN | 294 | Power Door Lock Motor Unlock
2 | GY | 295 | Power Door Lock Motor Lock | 2 | GY | 294 | Power Door Lock Motor Lock
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | D-BU | 1307 | Ignition 1 Voltage | 4 | D-BU | 1307 | Ignition 1 Voltage
5 | PU | 171 | Power Window Switch Down | 5 | PU | 171 | Power Window Switch Down
6 | L-GN | 170 | Power Window Switch Up | 6 | L-GN | 170 | Power Window Switch Up

### C401 Liftgate Harness to Floor Harness

#### Connector Part Information

- OEM: 936230-1
- Service: N/A
- Description: 6-Way F 090 II Series (NA)

#### Connector Part Information

- OEM: 936240-1
- Service: N/A
- Description: 6-Way M 090 Series (NA)

#### C401 Liftgate Harness to Floor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | PU | 293 | Rear Defogger | 1 | PU | 293 | Rear Defogger
2 | YE | 804 | Liftgate Switch | 2 | YE | 804 | Liftgate Switch
3 | PU | 709 | License Lamp | 3 | PU | 709 | License Lamp
4 | L-BU/D-BU | 20 | Center High Mount Stop Lamp (CHMSL) | 4 | L-BU/D-BU | 20 | Center High Mount Stop Lamp (CHMSL)
5 | GY/WH | 391 | Rear Wiper Signal | 5 | GY/WH | 391 | Rear Wiper Signal
6 | BN/YE | 141 | Rear Wiper Battery Voltage | 6 | BN/YE | 141 | Rear Wiper Battery Voltage